(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PI7C9X3G606GP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 49.53 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PI7C9X3G606GP"
				(at 49.53 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PI7C9X3G606GP"
				(at 49.53 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PI7C9X3G606GP.pdf"
				(at 49.53 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "6-Port 6-Lane PCI Express Gen 3 Switch, 10mm x 10mm FC-LFBGA (144 Pin) 0.8mm pitch"
				(at 49.53 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PI7C9X3G606GPCFCAEX"
				(at 49.53 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diodes Incorporated"
				(at 49.53 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 49.53 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 49.53 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "PCIE, SWITCH, IC, BGA"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PI7C9X3G606GP_1_1"
				(pin output line
					(at 35.56 -2.54 180)
					(length 3.81)
					(name "REFCLKO1_N")
					(number "A1")
				)
				(pin output line
					(at 35.56 0 180)
					(length 3.81)
					(name "REFCLKO1_P")
					(number "A2")
				)
				(pin output line
					(at 35.56 -8.89 180)
					(length 3.81)
					(name "REFCLKO4_N")
					(number "A3")
				)
				(pin output line
					(at 35.56 -6.35 180)
					(length 3.81)
					(name "REFCLKO4_P")
					(number "A4")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "REFCLKI0_N")
					(number "A5")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "REFCLKI0_P")
					(number "A6")
				)
				(pin input line
					(at 0 -59.69 0)
					(length 3.81)
					(name "PER1_N")
					(number "A7")
				)
				(pin input line
					(at 0 -57.15 0)
					(length 3.81)
					(name "PER1_P")
					(number "A8")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PER0_N")
					(number "A9")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PER0_P")
					(number "A10")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 3.81)
					(name "~{PERST}")
					(number "A12")
				)
				(pin output line
					(at 35.56 -19.05 180)
					(length 3.81)
					(name "REFCLKO6_P")
					(number "B2")
				)
				(pin output line
					(at 35.56 -12.7 180)
					(length 3.81)
					(name "REFCLKO5_P")
					(number "B3")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "~{CLKREQ7}")
					(number "B5")
					(alternate "GPIO15" bidirectional line)
				)
				(pin output line
					(at 35.56 -25.4 180)
					(length 3.81)
					(name "REFCLKO7_P")
					(number "C1")
				)
				(pin output line
					(at 35.56 -21.59 180)
					(length 3.81)
					(name "REFCLKO6_N")
					(number "C2")
				)
				(pin output line
					(at 35.56 -15.24 180)
					(length 3.81)
					(name "REFCLKO5_N")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "~{CLKREQ5}")
					(number "C4")
					(alternate "GPIO13" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "~{CLKREQ6}")
					(number "C5")
					(alternate "GPIO14" bidirectional line)
				)
				(pin input line
					(at 0 -16.51 0)
					(length 3.81)
					(name "RESREF")
					(number "C6")
				)
				(pin output line
					(at 0 -54.61 0)
					(length 3.81)
					(name "PET1_N")
					(number "C7")
				)
				(pin output line
					(at 0 -52.07 0)
					(length 3.81)
					(name "PET1_P")
					(number "C8")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PET0_N")
					(number "C9")
				)
				(pin output line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PET0_P")
					(number "C10")
				)
				(pin output line
					(at 35.56 -27.94 180)
					(length 3.81)
					(name "REFCLKO7_N")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "~{CLKREQ4}")
					(number "D3")
					(alternate "GPIO12" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "~{CLKREQ0}")
					(number "E3")
					(alternate "GPIO8" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "~{CLKREQ1}")
					(number "E4")
					(alternate "GPIO9" bidirectional line)
				)
				(pin output line
					(at 0 -63.5 0)
					(length 3.81)
					(name "PET2_P")
					(number "K3")
				)
				(pin output line
					(at 0 -66.04 0)
					(length 3.81)
					(name "PET2_N")
					(number "K4")
				)
				(pin output line
					(at 35.56 -40.64 180)
					(length 3.81)
					(name "PET3_P")
					(number "K5")
				)
				(pin output line
					(at 35.56 -43.18 180)
					(length 3.81)
					(name "PET3_N")
					(number "K6")
				)
				(pin output line
					(at 35.56 -52.07 180)
					(length 3.81)
					(name "PET4_P")
					(number "K7")
				)
				(pin output line
					(at 35.56 -54.61 180)
					(length 3.81)
					(name "PET4_N")
					(number "K8")
				)
				(pin output line
					(at 35.56 -68.58 180)
					(length 3.81)
					(name "PET5_P")
					(number "K9")
				)
				(pin output line
					(at 35.56 -71.12 180)
					(length 3.81)
					(name "PET5_N")
					(number "K10")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 3.81)
					(name "REFCLKI1_P")
					(number "L6")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 3.81)
					(name "REFCLKI1_N")
					(number "L7")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 3.81)
					(name "PER2_P")
					(number "M3")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 3.81)
					(name "PER2_N")
					(number "M4")
				)
				(pin input line
					(at 35.56 -45.72 180)
					(length 3.81)
					(name "PER3_P")
					(number "M5")
				)
				(pin input line
					(at 35.56 -48.26 180)
					(length 3.81)
					(name "PER3_N")
					(number "M6")
				)
				(pin input line
					(at 35.56 -57.15 180)
					(length 3.81)
					(name "PER4_P")
					(number "M7")
				)
				(pin input line
					(at 35.56 -59.69 180)
					(length 3.81)
					(name "PER4_N")
					(number "M8")
				)
				(pin input line
					(at 35.56 -63.5 180)
					(length 3.81)
					(name "PER5_P")
					(number "M9")
				)
				(pin input line
					(at 35.56 -66.04 180)
					(length 3.81)
					(name "PER5_N")
					(number "M10")
				)
			)
			(symbol "PI7C9X3G606GP_2_1"
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "EEDO")
					(number "J12")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "EECK")
					(number "K12")
				)
				(pin output line
					(at 22.86 0 180)
					(length 3.81)
					(name "EEDI")
					(number "L11")
				)
				(pin output line
					(at 22.86 -6.35 180)
					(length 3.81)
					(name "SCL_I2C")
					(number "L12")
				)
				(pin output line
					(at 22.86 -2.54 180)
					(length 3.81)
					(name "~{EECS}")
					(number "M11")
				)
				(pin bidirectional line
					(at 22.86 -8.89 180)
					(length 3.81)
					(name "SDA_I2C")
					(number "M12")
				)
			)
			(symbol "PI7C9X3G606GP_3_1"
				(pin input line
					(at 0 -44.45 0)
					(length 3.81)
					(name "PORTCFG0")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "GPIO0")
					(number "B12")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 3.81)
					(name "PORTCFG1")
					(number "C11")
				)
				(pin output line
					(at 33.02 -7.62 180)
					(length 3.81)
					(name "HP_LED1")
					(number "C12")
					(alternate "GPIO1" bidirectional line)
				)
				(pin input line
					(at 0 -54.61 0)
					(length 3.81)
					(name "CKMODE")
					(number "D9")
				)
				(pin input line
					(at 0 -49.53 0)
					(length 3.81)
					(name "PORTCFG2")
					(number "D11")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "GPIO2")
					(number "D12")
				)
				(pin input line
					(at 33.02 -60.96 180)
					(length 3.81)
					(name "~{PM_L11_EN}")
					(number "E1")
					(alternate "~{INTA}" output line)
				)
				(pin output line
					(at 33.02 -54.61 180)
					(length 3.81)
					(name "TEST")
					(number "E2")
				)
				(pin input line
					(at 33.02 -58.42 180)
					(length 3.81)
					(name "~{HOT_PLUG_EN}")
					(number "E9")
					(alternate "~{FATAL_ERR}" output line)
				)
				(pin output line
					(at 33.02 -40.64 180)
					(length 3.81)
					(name "~{PORTGOOD1}")
					(number "E10")
				)
				(pin output line
					(at 33.02 -38.1 180)
					(length 3.81)
					(name "~{PORTGOOD0}")
					(number "E11")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "GPIO3")
					(number "E12")
				)
				(pin output line
					(at 33.02 -17.78 180)
					(length 3.81)
					(name "HP_LED7")
					(number "F1")
					(alternate "GPIO7" bidirectional line)
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "~{PDC7}")
					(number "F2")
				)
				(pin output line
					(at 33.02 -30.48 180)
					(length 3.81)
					(name "~{HP_RST6}")
					(number "F3")
					(alternate "GPIO22" bidirectional line)
				)
				(pin output line
					(at 33.02 -27.94 180)
					(length 3.81)
					(name "~{HP_RST5}")
					(number "F4")
					(alternate "GPIO21" bidirectional line)
				)
				(pin input line
					(at 0 -38.1 0)
					(length 3.81)
					(name "CHIP_MODE0")
					(number "F9")
				)
				(pin output line
					(at 33.02 -45.72 180)
					(length 3.81)
					(name "~{PORTGOOD5}")
					(number "F10")
				)
				(pin output line
					(at 33.02 -10.16 180)
					(length 3.81)
					(name "HP_LED4")
					(number "F12")
					(alternate "GPIO4" bidirectional line)
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "~{PDC6}")
					(number "G1")
				)
				(pin output line
					(at 33.02 -22.86 180)
					(length 3.81)
					(name "~{HP_RST1}")
					(number "G2")
					(alternate "GPIO17" bidirectional line)
				)
				(pin output line
					(at 33.02 -25.4 180)
					(length 3.81)
					(name "~{HP_RST4}")
					(number "G3")
					(alternate "GPIO20" bidirectional line)
				)
				(pin output line
					(at 33.02 -33.02 180)
					(length 3.81)
					(name "~{HP_RST7}")
					(number "G4")
					(alternate "GPIO23" output line)
				)
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "CHIP_MODE1")
					(number "G9")
				)
				(pin output line
					(at 33.02 -48.26 180)
					(length 3.81)
					(name "~{PORTGOOD6}")
					(number "G10")
				)
				(pin output line
					(at 33.02 -43.18 180)
					(length 3.81)
					(name "~{PORTGOOD4}")
					(number "G11")
				)
				(pin output line
					(at 33.02 -12.7 180)
					(length 3.81)
					(name "HP_LED5")
					(number "G12")
					(alternate "GPIO5" bidirectional line)
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "~{PDC5}")
					(number "H1")
				)
				(pin no_connect line
					(at 3.81 -57.15 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H2")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "GPIO18")
					(number "H3")
				)
				(pin no_connect line
					(at 3.81 -58.42 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H4")
				)
				(pin output line
					(at 33.02 -50.8 180)
					(length 3.81)
					(name "~{PORTGOOD7}")
					(number "H11")
				)
				(pin output line
					(at 33.02 -15.24 180)
					(length 3.81)
					(name "HP_LED6")
					(number "H12")
					(alternate "GPIO6" bidirectional line)
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "~{PDC4}")
					(number "J1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "~{PDC1}")
					(number "J2")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "GPIO19")
					(number "J4")
				)
				(pin no_connect line
					(at 3.81 -59.69 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K1")
				)
				(pin output line
					(at 33.02 0 180)
					(length 3.81)
					(name "SHCL_I2C")
					(number "L1")
				)
				(pin no_connect line
					(at 3.81 -60.96 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L2")
				)
				(pin bidirectional line
					(at 33.02 -2.54 180)
					(length 3.81)
					(name "SHDA_I2C")
					(number "M1")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "~{SHPCINT}")
					(number "M2")
				)
			)
			(symbol "PI7C9X3G606GP_4_1"
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(name "VSS")
					(number "B1")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "B4")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "B6")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "B7")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "B8")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "B9")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "B10")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 3.81)
					(name "C_VDDR")
					(number "D2")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "C_VDDC")
					(number "D4")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "D5")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E6")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E8")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F5")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F7")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F11")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G6")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G8")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H5")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H7")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J8")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K2")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K11")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L3")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L4")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L5")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L8")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L9")
				)
				(pin passive line
					(at 20.32 -27.94 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L10")
				)
				(pin power_in line
					(at 0 -21.59 0)
					(length 3.81)
					(name "VP")
					(number "[D6,D7,J6,J7]")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 3.81)
					(name "VPH")
					(number "[D8,J5]")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 3.81)
					(name "VDDR")
					(number "[D10,J3]")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDDC")
					(number "[E5,E7,F6,F8,G5,G7,H6,H8]")
				)
			)
			(symbol "PI7C9X3G606GP_5_1"
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "~{JTAG_SEL}")
					(number "A11")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "TCK")
					(number "H9")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "TMS")
					(number "H10")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "~{TRST}")
					(number "J9")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "TDI")
					(number "J10")
				)
				(pin output line
					(at 27.94 0 180)
					(length 3.81)
					(name "TDO")
					(number "J11")
				)
			)
			(embedded_fonts no)
		)
)
