(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PF9455"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 58.42 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PF9455"
				(at 58.42 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PF9455"
				(at 58.42 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/product-brief/PF9455_PB.pdf"
				(at 58.42 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Highly optimized PMIC for functionally safe and quality managed i.MX9 MPU‑based applications"
				(at 58.42 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PPF9455AVMA7ES"
				(at 58.42 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "NXP"
				(at 58.42 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 58.42 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 58.42 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC, CONTROLLER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PF9455_1_1"
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "STBY")
					(number "1")
				)
				(pin power_in line
					(at 0 -50.8 0)
					(length 2.54)
					(name "LDO2IN")
					(number "2")
				)
				(pin power_out line
					(at 43.18 -53.34 180)
					(length 2.54)
					(name "LDO2OUT")
					(number "3")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 2.54)
					(name "FCCU0")
					(number "4")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SW3IN")
					(number "5")
				)
				(pin power_out line
					(at 43.18 -20.32 180)
					(length 2.54)
					(name "SW3LXA")
					(number "6")
				)
				(pin power_out line
					(at 43.18 -22.86 180)
					(length 2.54)
					(name "SW3LXB")
					(number "7")
				)
				(pin power_out line
					(at 43.18 -12.7 180)
					(length 2.54)
					(name "SW2LXB")
					(number "8")
				)
				(pin power_out line
					(at 43.18 -10.16 180)
					(length 2.54)
					(name "SW2LXA")
					(number "9")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 2.54)
					(name "SW2IN")
					(number "10")
				)
				(pin no_connect line
					(at 40.64 -93.98 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "11")
				)
				(pin power_out line
					(at 43.18 -55.88 180)
					(length 2.54)
					(name "LDO3OUT")
					(number "12")
				)
				(pin power_in line
					(at 0 -53.34 0)
					(length 2.54)
					(name "LDO3IN")
					(number "13")
				)
				(pin bidirectional line
					(at 43.18 -68.58 180)
					(length 2.54)
					(name "XFAILB")
					(number "14")
				)
				(pin output line
					(at 43.18 -73.66 180)
					(length 2.54)
					(name "AMUX")
					(number "15")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VAON")
					(number "16")
				)
				(pin no_connect line
					(at 40.64 -91.44 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "18")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VDDOTP")
					(number "19")
				)
				(pin input line
					(at 43.18 -15.24 180)
					(length 2.54)
					(name "SW2FB")
					(number "20")
				)
				(pin input line
					(at 43.18 -25.4 180)
					(length 2.54)
					(name "SW3FB")
					(number "21")
				)
				(pin input line
					(at 43.18 -45.72 180)
					(length 2.54)
					(name "SW5FB")
					(number "22")
				)
				(pin input line
					(at 43.18 -35.56 180)
					(length 2.54)
					(name "SW4FB")
					(number "23")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 2.54)
					(name "DGND")
					(number "24")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDIG")
					(number "25")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VANA")
					(number "26")
				)
				(pin passive line
					(at 0 -93.98 0)
					(length 2.54)
					(name "AGND")
					(number "27")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PWRON")
					(number "28")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VMON1")
					(number "29")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VMON2")
					(number "30")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 2.54)
					(name "SW4IN")
					(number "31")
				)
				(pin power_out line
					(at 43.18 -30.48 180)
					(length 2.54)
					(name "SW4LXA")
					(number "32")
				)
				(pin power_out line
					(at 43.18 -33.02 180)
					(length 2.54)
					(name "SW4LXB")
					(number "33")
				)
				(pin power_out line
					(at 43.18 -43.18 180)
					(length 2.54)
					(name "SW5LXB")
					(number "34")
				)
				(pin power_out line
					(at 43.18 -40.64 180)
					(length 2.54)
					(name "SW5LXA")
					(number "35")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 2.54)
					(name "SW5IN")
					(number "36")
				)
				(pin power_out line
					(at 43.18 -2.54 180)
					(length 2.54)
					(name "SW1LXB")
					(number "37")
				)
				(pin power_out line
					(at 43.18 0 180)
					(length 2.54)
					(name "SW1LXA")
					(number "38")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 2.54)
					(name "SW1INB")
					(number "39")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 2.54)
					(name "SW1INA")
					(number "40")
				)
				(pin output line
					(at 43.18 -66.04 180)
					(length 2.54)
					(name "INTB")
					(number "41")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 2.54)
					(name "FSYNC")
					(number "42")
				)
				(pin output line
					(at 43.18 -63.5 180)
					(length 2.54)
					(name "RSTB")
					(number "43")
				)
				(pin output line
					(at 43.18 -60.96 180)
					(length 2.54)
					(name "PGOOD")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 2.54)
					(name "GPIO1")
					(number "45")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 2.54)
					(name "GPIO2")
					(number "46")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 2.54)
					(name "FCCU1")
					(number "47")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDDIO")
					(number "48")
				)
				(pin input line
					(at 43.18 -5.08 180)
					(length 2.54)
					(name "SW1FB")
					(number "49")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "SDA")
					(number "50")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "SCL")
					(number "51")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 2.54)
					(name "LDO1IN")
					(number "52")
				)
				(pin power_out line
					(at 43.18 -50.8 180)
					(length 2.54)
					(name "LDO1OUT")
					(number "53")
				)
				(pin output line
					(at 43.18 -71.12 180)
					(length 2.54)
					(name "FS0B")
					(number "54")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 2.54)
					(name "GPIO3")
					(number "55")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 2.54)
					(name "GPIO4")
					(number "56")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 2.54)
					(name "EPAD")
					(number "57")
				)
			)
			(embedded_fonts no)
		)
)
