(footprint "QFN-56-1EP_8x8mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "QFN 56 Pin")
	(tags "QFN")
	(property "Reference" "REF**"
		(at 0 -5.321 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-56-1EP_8x8mm_P0.5mm"
		(at 0 5.32 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -4.4 7.32 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.4 8.519 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.4 9.719 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -2.101 -2.101)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at -2.101 -0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at -2.101 0.699)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at -2.101 2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at -0.7 -2.101)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at -0.7 -0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at -0.7 0.699)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at -0.7 2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 0.699 -2.101)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 0.699 -0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 0.699 0.699)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 0.699 2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 2.1 -2.101)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 2.1 -0.7)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 2.1 0.699)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 2.1 2.1)
		(size 1.13 1.13)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "1" smd roundrect
		(at -3.938 -3.25)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.938 -2.75)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.938 -2.25)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.938 -1.75)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -3.938 -1.25)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -3.938 -0.75)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -3.938 -0.25)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -3.938 0.249)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -3.938 0.749)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -3.938 1.249)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -3.938 1.749)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -3.938 2.249)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -3.938 2.749)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -3.938 3.249)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at -3.25 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at -2.75 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at -2.25 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at -1.75 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at -1.25 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at -0.75 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at -0.25 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 0.249 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 0.749 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 1.249 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 1.749 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 2.249 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 2.749 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 3.249 3.937 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 3.937 3.249)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 3.937 2.749)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 3.937 2.249)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 3.937 1.749)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 3.937 1.249)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 3.937 0.749)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at 3.937 0.249)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at 3.937 -0.25)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at 3.937 -0.75)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at 3.937 -1.25)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at 3.937 -1.75)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at 3.937 -2.25)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at 3.937 -2.75)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "42" smd roundrect
		(at 3.937 -3.25)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "43" smd roundrect
		(at 3.249 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "44" smd roundrect
		(at 2.749 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "45" smd roundrect
		(at 2.249 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "46" smd roundrect
		(at 1.749 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "47" smd roundrect
		(at 1.249 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "48" smd roundrect
		(at 0.749 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "49" smd roundrect
		(at 0.249 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "50" smd roundrect
		(at -0.25 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "51" smd roundrect
		(at -0.75 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "52" smd roundrect
		(at -1.25 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "53" smd roundrect
		(at -1.75 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "54" smd roundrect
		(at -2.25 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "55" smd roundrect
		(at -2.75 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "56" smd roundrect
		(at -3.25 -3.938 90)
		(size 0.875 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "57" smd rect
		(at 0 0)
		(size 5.9 5.9)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_ppf9455avsa4es.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
