(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PPF9455AVSA4ES"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 37.338 -1.778 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PPF9455AVSA4ES"
				(at 37.338 -6.858 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PPF9455AVSA4ES"
				(at 37.338 -9.398 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/product-brief/PF9455_PB.pdf"
				(at 37.338 -11.938 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "9-Channel PMIC for i.MX94 based applications"
				(at 37.338 -24.638 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "NXP"
				(at 37.338 -17.018 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PPF9455AVSA4ES"
				(at 37.338 -4.318 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 37.338 -19.558 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 37.338 -22.098 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, VOLTAGE, REGULATOR, SWITCHING, DC-DC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PPF9455AVSA4ES_1_1"
				(pin passive line
					(at 0 -166.37 0)
					(length 2.54)
					(name "STBY")
					(number "1")
				)
				(pin passive line
					(at 0 -85.09 0)
					(length 2.54)
					(name "LDO2IN")
					(number "2")
				)
				(pin passive line
					(at 26.67 -85.09 180)
					(length 2.54)
					(name "LDO2OUT")
					(number "3")
				)
				(pin passive line
					(at 0 -156.21 0)
					(length 2.54)
					(name "FCCU0")
					(number "4")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "SW3IN")
					(number "5")
				)
				(pin passive line
					(at 26.67 -33.02 180)
					(length 2.54)
					(name "SW3LX")
					(number "6")
				)
				(pin passive line
					(at 26.67 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "SW3LX")
					(number "7")
				)
				(pin passive line
					(at 26.67 -16.51 180)
					(length 2.54)
					(name "SW2LX")
					(number "8")
				)
				(pin passive line
					(at 26.67 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "SW2LX")
					(number "9")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 2.54)
					(name "SW2IN")
					(number "10")
				)
				(pin no_connect line
					(at 2.54 -96.52 0)
					(length 2.54)
					(hide yes)
					(name "NC1")
					(number "11")
				)
				(pin passive line
					(at 26.67 -87.63 180)
					(length 2.54)
					(name "LDO3OUT")
					(number "12")
				)
				(pin passive line
					(at 0 -87.63 0)
					(length 2.54)
					(name "LDO3IN")
					(number "13")
				)
				(pin passive line
					(at 26.67 -158.75 180)
					(length 2.54)
					(name "XFAILB")
					(number "14")
				)
				(pin passive line
					(at 26.67 -137.16 180)
					(length 2.54)
					(name "AMUX")
					(number "15")
				)
				(pin passive line
					(at 26.67 -102.87 180)
					(length 2.54)
					(name "VAON")
					(number "16")
				)
				(pin no_connect line
					(at 2.54 -99.06 0)
					(length 2.54)
					(hide yes)
					(name "NC2")
					(number "17")
				)
				(pin passive line
					(at 0 -107.95 0)
					(length 2.54)
					(name "VIN")
					(number "18")
				)
				(pin passive line
					(at 26.67 -121.92 180)
					(length 2.54)
					(name "VDDOTP")
					(number "19")
				)
				(pin passive line
					(at 26.67 -22.86 180)
					(length 2.54)
					(name "SW2FB")
					(number "20")
				)
				(pin passive line
					(at 26.67 -39.37 180)
					(length 2.54)
					(name "SW3FB")
					(number "21")
				)
				(pin passive line
					(at 26.67 -72.39 180)
					(length 2.54)
					(name "SW5FB")
					(number "22")
				)
				(pin passive line
					(at 26.67 -55.88 180)
					(length 2.54)
					(name "SW4FB")
					(number "23")
				)
				(pin passive line
					(at 26.67 -171.45 180)
					(length 2.54)
					(name "DGND")
					(number "24")
				)
				(pin passive line
					(at 26.67 -107.95 180)
					(length 2.54)
					(name "VDIG")
					(number "25")
				)
				(pin passive line
					(at 26.67 -105.41 180)
					(length 2.54)
					(name "VANA")
					(number "26")
				)
				(pin passive line
					(at 26.67 -168.91 180)
					(length 2.54)
					(name "AGND")
					(number "27")
				)
				(pin passive line
					(at 0 -168.91 0)
					(length 2.54)
					(name "PWRON")
					(number "28")
				)
				(pin passive line
					(at 26.67 -161.29 180)
					(length 2.54)
					(name "VMON1")
					(number "29")
				)
				(pin passive line
					(at 26.67 -163.83 180)
					(length 2.54)
					(name "VMON2")
					(number "30")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 2.54)
					(name "SW4IN")
					(number "31")
				)
				(pin passive line
					(at 26.67 -49.53 180)
					(length 2.54)
					(name "SW4LX")
					(number "32")
				)
				(pin passive line
					(at 26.67 -49.53 180)
					(length 2.54)
					(hide yes)
					(name "SW4LX")
					(number "33")
				)
				(pin passive line
					(at 26.67 -66.04 180)
					(length 2.54)
					(name "SW5LX")
					(number "34")
				)
				(pin passive line
					(at 26.67 -66.04 180)
					(length 2.54)
					(hide yes)
					(name "SW5LX")
					(number "35")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "SW5IN")
					(number "36")
				)
				(pin passive line
					(at 26.67 0 180)
					(length 2.54)
					(name "SW1LX")
					(number "37")
				)
				(pin passive line
					(at 26.67 0 180)
					(length 2.54)
					(hide yes)
					(name "SW1LX")
					(number "38")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "SW1IN")
					(number "39")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "SW1IN")
					(number "40")
				)
				(pin passive line
					(at 0 -137.16 0)
					(length 2.54)
					(name "INTB")
					(number "41")
				)
				(pin passive line
					(at 0 -173.99 0)
					(length 2.54)
					(name "FSYNC")
					(number "42")
				)
				(pin passive line
					(at 0 -163.83 0)
					(length 2.54)
					(name "RSTB")
					(number "43")
				)
				(pin passive line
					(at 0 -142.24 0)
					(length 2.54)
					(name "PGOOD")
					(number "44")
				)
				(pin passive line
					(at 26.67 -139.7 180)
					(length 2.54)
					(name "GPIO1")
					(number "45")
				)
				(pin passive line
					(at 26.67 -142.24 180)
					(length 2.54)
					(name "GPIO2")
					(number "46")
				)
				(pin passive line
					(at 0 -158.75 0)
					(length 2.54)
					(name "FCCU1")
					(number "47")
				)
				(pin passive line
					(at 0 -121.92 0)
					(length 2.54)
					(name "VDDIO")
					(number "48")
				)
				(pin passive line
					(at 26.67 -6.35 180)
					(length 2.54)
					(name "SW1FB")
					(number "49")
				)
				(pin passive line
					(at 0 -151.13 0)
					(length 2.54)
					(name "SDA")
					(number "50")
				)
				(pin passive line
					(at 0 -148.59 0)
					(length 2.54)
					(name "SCL")
					(number "51")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 2.54)
					(name "LDO1IN")
					(number "52")
				)
				(pin passive line
					(at 26.67 -82.55 180)
					(length 2.54)
					(name "LDO1OUT")
					(number "53")
				)
				(pin passive line
					(at 0 -139.7 0)
					(length 2.54)
					(name "FS0B")
					(number "54")
				)
				(pin passive line
					(at 26.67 -144.78 180)
					(length 2.54)
					(name "GPIO3")
					(number "55")
				)
				(pin passive line
					(at 26.67 -147.32 180)
					(length 2.54)
					(name "GPIO4")
					(number "56")
				)
				(pin passive line
					(at 26.67 -173.99 180)
					(length 2.54)
					(name "EPAD(GND)")
					(number "57")
				)
			)
			(embedded_fonts no)
		)
)
