(footprint "SW_SDA04H1SBD_SMD"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -6.6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "SW_SDA04H1SBD_SMD"
		(at 0 7.4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -6.44 9.95 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -6.44 11.15 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -6.44 12.35 0)
		(layer "F.Fab")
	)
	(pad "A1" smd rect
		(at -4.115 -3.77 270)
		(size 1.5 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd rect
		(at -4.115 -1.23 270)
		(size 1.5 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd rect
		(at -4.115 1.31 270)
		(size 1.5 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd rect
		(at -4.115 3.85 270)
		(size 1.5 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd rect
		(at 4.135 -3.77 270)
		(size 1.5 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd rect
		(at 4.135 -1.23 270)
		(size 1.5 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd rect
		(at 4.135 1.31 270)
		(size 1.5 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd rect
		(at 4.135 3.85 270)
		(size 1.5 2.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_sda04h1sbd.glb"
		(offset
			(xyz 0 6 2.75)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 180)
		)
	)
)
