(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SIC431AED-T1-GE3"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SIC431AED-T1-GE3"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SIC431AED-T1-GE3"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.vishay.com/docs/74589/sic431.pdf"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC/DC Synchronous Regulator, Adjustable, 3V to 24VIn, 0.6V to 22V/24AOut, 1MHz, MLP44-24L"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Vishay"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SIC431AED-T1-GE3 "
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, DC-DC, CONVERTER, SWITCHING, VOLTAGE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SIC431AED-T1-GE3_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{IN}")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "V_{IN}")
					(number "2")
				)
				(pin passive line
					(at 21.59 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "P_{GND}")
					(number "3")
				)
				(pin passive line
					(at 21.59 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "P_{GND}")
					(number "4")
				)
				(pin passive line
					(at 21.59 -5.08 180)
					(length 2.54)
					(name "SW")
					(number "5")
				)
				(pin passive line
					(at 21.59 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "6")
				)
				(pin passive line
					(at 21.59 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "7")
				)
				(pin passive line
					(at 21.59 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "8")
				)
				(pin passive line
					(at 21.59 -5.08 180)
					(length 2.54)
					(hide yes)
					(name "SW")
					(number "9")
				)
				(pin passive line
					(at 21.59 -7.62 180)
					(length 2.54)
					(name "GL")
					(number "10")
				)
				(pin passive line
					(at 21.59 -7.62 180)
					(length 2.54)
					(hide yes)
					(name "GL")
					(number "11")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "V_{DRV}")
					(number "12")
				)
				(pin power_in line
					(at 21.59 -20.32 180)
					(length 2.54)
					(name "P_{GND}")
					(number "13")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 2.54)
					(name "P_{GOOD}")
					(number "14")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "V_{DD}")
					(number "15")
				)
				(pin power_in line
					(at 21.59 -17.78 180)
					(length 2.54)
					(name "A_{GND}")
					(number "16")
				)
				(pin passive line
					(at 21.59 -12.7 180)
					(length 2.54)
					(name "FB")
					(number "17")
				)
				(pin passive line
					(at 21.59 -10.16 180)
					(length 2.54)
					(name "V_{OUT}")
					(number "18")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "EN")
					(number "19")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "MODE2")
					(number "20")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "MODE1")
					(number "21")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "V_{IN}")
					(number "22")
				)
				(pin passive line
					(at 21.59 0 180)
					(length 2.54)
					(name "BOOT")
					(number "23")
				)
				(pin passive line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "PHASE")
					(number "24")
				)
				(pin passive line
					(at 21.59 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "A_{GND}")
					(number "25")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "V_{IN}")
					(number "26")
				)
				(pin passive line
					(at 21.59 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "P_{GND}")
					(number "27")
				)
				(pin passive line
					(at 21.59 -7.62 180)
					(length 2.54)
					(hide yes)
					(name "GL")
					(number "28")
				)
			)
			(embedded_fonts no)
		)
)
