(footprint "SIC47XED-T1-GE3"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "SIC47XED-T1-GE3"
		(at 0 4.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -4.851 5.94 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.851 7.14 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.851 8.339 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.525 -1.7)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.525 -1.051)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.525 -0.403)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.525 0.247)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.525 1.249)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.525 1.749)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.52 2.523)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -1.2 0.997)
		(size 1.1 2.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "8" smd rect
		(at -0.87 2.523)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.26 2.523)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.409 0.997)
		(size 1.52 2.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at 0.699 1.485)
		(size 2.1 1.73)
		(layers "F.Cu" "F.Mask")
	)
	(pad "10" smd rect
		(at 0.757 2.523)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.259 2.523)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 2.523 1.898)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.523 1.398)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.2 1.398)
		(size 0.3 1.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.523 0.9)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 2.523 0.247)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 2.523 -0.25)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 2.523 -0.75)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 2.523 -1.25)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 2.523 -1.75)
		(size 0.95 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 1.749 -2.525)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 1.249 -2.525)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 0.747 -2.525)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 0.247 -2.525)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -0.25 -2.525)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -0.75 -2.525)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -1.25 -2.525)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -1.75 -2.525)
		(size 0.35 0.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 0 -1.2)
		(size 3.4 1.1)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_sic477ed_t1_ge3.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
