(footprint "RENESAS-TDFN-8-1.5x2.0mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "8 Lead TDFN Package 1.5 x 2.0 mm (Fused Lead) JEDEC MO-252 ")
	(property "Reference" "REF**"
		(at -1.4 -1.6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "RENESAS-TDFN-8-1.5x2.0mm_P0.5mm"
		(at -9.7 2.4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -9.7 4.4 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -9.7 5.6 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -9.7 6.8 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.527 -0.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.576 -0.25 270)
		(size 0.28 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd custom
		(at -0.576 0.248 270)
		(size 0.28 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.14 -0.375) (xy -0.14 0.05) (xy 0.64 0.05) (xy 0.64 -0.375)
				)
				(width 0)
				(fill yes)
			)
			(gr_rect
				(start 0.36 -0.375)
				(end 0.64 0.375)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "5" smd custom
		(at 0.574 0.748 90)
		(size 0.28 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.14 -0.375) (xy -0.14 0.05) (xy 0.64 0.05) (xy 0.64 -0.375)
				)
				(width 0)
				(fill yes)
			)
			(gr_rect
				(start 0.36 -0.375)
				(end 0.64 0.375)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "7" smd rect
		(at 0.574 -0.25 270)
		(size 0.28 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.574 -0.75 270)
		(size 0.28 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_slg59m1457v.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
