(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "SN3257QDYYRQ1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 41.91 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "SN3257QDYYRQ1"
				(at 41.91 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "SN3257QDYYRQ1"
				(at 41.91 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn3257-q1.pdf?ts=1730807589044&ref_url=https%253A%252F%252Fwww.mouser.fr%252F"
				(at 41.91 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Interface analog switch/multiplexer/demultiplexer"
				(at 41.91 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SN3257QDYYRQ1"
				(at 41.91 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 41.91 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 41.91 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS, SWITCH"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "SN3257QDYYRQ1_1_1"
				(pin input line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "SEL")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "S1A")
					(number "2")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "S1B")
					(number "3")
				)
				(pin passive line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "D1")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "S2A")
					(number "5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "S2B")
					(number "6")
				)
				(pin passive line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "D2")
					(number "7")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GND")
					(number "8")
				)
				(pin passive line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "D3")
					(number "9")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "S3B")
					(number "10")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "S3A")
					(number "11")
				)
				(pin passive line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "D4")
					(number "12")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "S4B")
					(number "13")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "S4A")
					(number "14")
				)
				(pin input line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "~{EN}")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
