(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STM6601DA2BDM6F"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STM6601DA2BDM6F"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STM6601DA2BDM6F"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm6600.pdf"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "STMICROELECTRONICS - STM6601CM2DDM6F - SMART PUSH-BUTTON ON/OFF CONTROL TDFN-12"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STM6601DA2BDM6F"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, CONTROLLER"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STM6601DA2BDM6F_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "1")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{SR}")
					(number "2")
				)
				(pin output line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "VREF")
					(number "3")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "PS_HOLD")
					(number "4")
				)
				(pin input line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "C_SRD")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{PB}")
					(number "6")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{VCCLO}")
					(number "7")
				)
				(pin output line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "~{PBOUT}")
					(number "8")
				)
				(pin output line
					(at 30.48 0 180)
					(length 2.54)
					(name "~{EN}")
					(number "9")
				)
				(pin output line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "~{RST}")
					(number "10")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "~{INT}")
					(number "11")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GND")
					(number "12")
				)
			)
			(embedded_fonts no)
		)
)
