(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TCA9548ARGER"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TCA9548ARGER"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TCA9548ARGER"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tca9548a.pdf?HQS=dis-dk-null-digikeymode-dsf-pf-null-wwe&ts=1691560939141&ref_url=https%253A%252F%252Fwww.mouser.com%252F"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Specialized Interface, I2C, SMBus, Servers & Routers, 1.65 V, 5.5 V, VQFN, 24 Pins"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TCA9548ARGER"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SWITCH, IC, LOGIC, SIGNAL, MUX, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TCA9548ARGER_1_1"
				(pin bidirectional line
					(at 20.32 0 180)
					(length 2.54)
					(name "SD0")
					(number "1")
				)
				(pin bidirectional line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "SC0")
					(number "2")
				)
				(pin bidirectional line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "SD1")
					(number "3")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "SC1")
					(number "4")
				)
				(pin bidirectional line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "SD2")
					(number "5")
				)
				(pin bidirectional line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "SC2")
					(number "6")
				)
				(pin bidirectional line
					(at 20.32 -22.86 180)
					(length 2.54)
					(name "SD3")
					(number "7")
				)
				(pin bidirectional line
					(at 20.32 -25.4 180)
					(length 2.54)
					(name "SC3")
					(number "8")
				)
				(pin power_in line
					(at 0 -55.88 0)
					(length 2.54)
					(name "GND")
					(number "9")
				)
				(pin bidirectional line
					(at 20.32 -30.48 180)
					(length 2.54)
					(name "SD4")
					(number "10")
				)
				(pin bidirectional line
					(at 20.32 -33.02 180)
					(length 2.54)
					(name "SC4")
					(number "11")
				)
				(pin bidirectional line
					(at 20.32 -38.1 180)
					(length 2.54)
					(name "SD5")
					(number "12")
				)
				(pin bidirectional line
					(at 20.32 -40.64 180)
					(length 2.54)
					(name "SC5")
					(number "13")
				)
				(pin bidirectional line
					(at 20.32 -45.72 180)
					(length 2.54)
					(name "SD6")
					(number "14")
				)
				(pin bidirectional line
					(at 20.32 -48.26 180)
					(length 2.54)
					(name "SC6")
					(number "15")
				)
				(pin bidirectional line
					(at 20.32 -53.34 180)
					(length 2.54)
					(name "SD7")
					(number "16")
				)
				(pin bidirectional line
					(at 20.32 -55.88 180)
					(length 2.54)
					(name "SC7")
					(number "17")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "A2")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SCL")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SDA")
					(number "20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "21")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "A0")
					(number "22")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "A1")
					(number "23")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "~{RESET}")
					(number "24")
				)
				(pin no_connect line
					(at 2.54 -53.34 0)
					(length 2.54)
					(hide yes)
					(name "EP")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
)
