(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TLK10232CTR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 46.99 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TLK10232CTR"
				(at 46.99 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TLK10232CTR"
				(at 46.99 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tlk10232.pdf?ts=1712150848075&ref_url=https%253A%252F%252Fwww.mouser.pl%252F"
				(at 46.99 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Dual channel XAUI-to-10GBASE-KR backplane transceiver with crosspoint switch"
				(at 46.99 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TLK10232CTR"
				(at 46.99 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 46.99 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 46.99 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 46.99 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, TRANSCEIVER, IC, ETHERNET, PHY"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TLK10232CTR_1_1"
				(text "CH A"
					(at 20.32 0 0)
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "INA1+")
					(number "A1")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "INA0-")
					(number "A3")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "INA0+")
					(number "A4")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 3.81)
					(name "OUTA0+")
					(number "A6")
				)
				(pin output line
					(at 0 -40.64 0)
					(length 3.81)
					(name "OUTA0-")
					(number "A7")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 3.81)
					(name "~{PDTRXA}")
					(number "A8")
				)
				(pin input line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "HSRXA-")
					(number "A12")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "INA1-")
					(number "B1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "INA2+")
					(number "B2")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 3.81)
					(name "OUTA1+")
					(number "B5")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 3.81)
					(name "OUTA1-")
					(number "B6")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 3.81)
					(name "LS_OK_{IN_A}")
					(number "B10")
				)
				(pin input line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "HSRXA+")
					(number "B12")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "INA2-")
					(number "C2")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 3.81)
					(name "OUTA2+")
					(number "C4")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 3.81)
					(name "OUTA2-")
					(number "C5")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "INA3+")
					(number "D1")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 3.81)
					(name "LS_OK_{OUT_A}")
					(number "D9")
				)
				(pin output line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "HSTXA+")
					(number "D12")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "INA3-")
					(number "E1")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 3.81)
					(name "OUTA3-")
					(number "E3")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 3.81)
					(name "LOSA")
					(number "E9")
				)
				(pin output line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "HSTXA-")
					(number "E12")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 3.81)
					(name "OUTA3+")
					(number "F3")
				)
			)
			(symbol "TLK10232CTR_2_1"
				(text "CH B\n"
					(at 20.32 0 0)
				)
				(pin input line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "HSRXB-")
					(number "G12")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "INB0+")
					(number "H1")
				)
				(pin output line
					(at 0 -40.64 0)
					(length 3.81)
					(name "OUTB0-")
					(number "H3")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 3.81)
					(name "LS_OK_{OUT_B}")
					(number "H9")
				)
				(pin input line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "HSRXB+")
					(number "H12")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "INB0-")
					(number "J1")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 3.81)
					(name "OUTB0+")
					(number "J3")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 3.81)
					(name "~{PDTRXB}")
					(number "J4")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "INB1+")
					(number "K2")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 3.81)
					(name "OUTB1-")
					(number "K4")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 3.81)
					(name "OUTB1+")
					(number "K5")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 3.81)
					(name "LOSB")
					(number "K8")
				)
				(pin output line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "HSTXB+")
					(number "K12")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "INB2+")
					(number "L1")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "INB1-")
					(number "L2")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 3.81)
					(name "OUTB2-")
					(number "L5")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 3.81)
					(name "OUTB2+")
					(number "L6")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 3.81)
					(name "LS_OK_{IN_B}")
					(number "L8")
				)
				(pin output line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "HSTXB-")
					(number "L12")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "INB2-")
					(number "M1")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "INB3+")
					(number "M3")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "INB3-")
					(number "M4")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 3.81)
					(name "OUTB3-")
					(number "M6")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 3.81)
					(name "OUTB3+")
					(number "M7")
				)
			)
			(symbol "TLK10232CTR_3_1"
				(text "MISC"
					(at 20.32 0 0)
				)
				(pin output line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "CLKOUTB+")
					(number "A9")
				)
				(pin output line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "CLKOUTB-")
					(number "A10")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 3.81)
					(name "TMS")
					(number "B8")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PRBSEN")
					(number "B9")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "TDI")
					(number "C8")
				)
				(pin output line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "CLKOUTA+")
					(number "C9")
				)
				(pin output line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "CLKOUTA-")
					(number "C10")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 3.81)
					(name "AMUXA")
					(number "C11")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 3.81)
					(name "AMUXB")
					(number "D4")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 3.81)
					(name "TDO")
					(number "D6")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "TCK")
					(number "D8")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 3.81)
					(name "~{TRST}")
					(number "E5")
				)
				(pin input line
					(at 30.48 -58.42 180)
					(length 3.81)
					(name "PRTAD0")
					(number "E10")
				)
				(pin input line
					(at 30.48 -55.88 180)
					(length 3.81)
					(name "PRTAD1")
					(number "G9")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "~{RESET}")
					(number "H5")
				)
				(pin input line
					(at 30.48 -43.18 180)
					(length 3.81)
					(name "MODE_{SEL}")
					(number "H10")
				)
				(pin input line
					(at 30.48 -50.8 180)
					(length 3.81)
					(name "PRTAD3")
					(number "J6")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "MDIO")
					(number "J7")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 3.81)
					(name "MDC")
					(number "J8")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PRBS_{PASS}")
					(number "J9")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 3.81)
					(name "GPI0")
					(number "J10")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "REFCLK1+")
					(number "K9")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "REFCLK1-")
					(number "K10")
				)
				(pin input line
					(at 30.48 -53.34 180)
					(length 3.81)
					(name "PRTAD2")
					(number "L9")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 3.81)
					(name "TESTEN")
					(number "L10")
				)
				(pin input line
					(at 30.48 -48.26 180)
					(length 3.81)
					(name "PRTAD4")
					(number "M8")
				)
				(pin input line
					(at 30.48 -40.64 180)
					(length 3.81)
					(name "ST")
					(number "M9")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "REFCLK0+")
					(number "M10")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "REFCLK0-")
					(number "M11")
				)
			)
			(symbol "TLK10232CTR_4_1"
				(text "POWER"
					(at 19.05 0 0)
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A2")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A5")
				)
				(pin power_in line
					(at 30.48 -30.48 180)
					(length 3.81)
					(name "GND")
					(number "A11")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B3")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B7")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B11")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C1")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VDDRA_{LS/HS}")
					(number "C3")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C6")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 3.81)
					(name "VDDO0")
					(number "C7")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDDA_{LS/HS}")
					(number "D2")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D3")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D5")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 3.81)
					(name "VPP")
					(number "D7")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D10")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D11")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E2")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E4")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "VDDD")
					(number "E6")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 3.81)
					(name "DVDD")
					(number "E7")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "VDDD")
					(number "E8")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "VDDRA_{LS/HS}")
					(number "E11")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDDA_{LS/HS}")
					(number "F2")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDDT_{LS/HS}")
					(number "F4")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F5")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "VDDD")
					(number "F6")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "DVDD")
					(number "F7")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDT_{LS/HS}")
					(number "F9")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F10")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDDA_{LS/HS}")
					(number "F11")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F12")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDDA_{LS/HS}")
					(number "G2")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDDT_{LS/HS}")
					(number "G4")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "DVDD")
					(number "G6")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "DVDD")
					(number "G8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDDA_{LS/HS}")
					(number "G10")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G11")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H2")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H4")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "VDDD")
					(number "H6")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "DVDD")
					(number "H7")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "VDDD")
					(number "H8")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H11")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDDA_{LS/HS}")
					(number "J2")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J5")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VDDRB_{LS/HS}")
					(number "J11")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J12")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "VDDRB_{LS/HS}")
					(number "K3")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K6")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 3.81)
					(name "VDDO1")
					(number "K7")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K11")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L3")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L4")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L7")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L11")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M2")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M5")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M12")
				)
			)
			(embedded_fonts no)
		)
)
