(footprint "UQFN-16-1.8x2.6mm_P0.4mm_Texas_RSV0016A"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "https://www.ti.com/lit/ds/symlink/sn74avch4t245-ep.pdf?ts=1679484181203&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FSN74AVCH4T245-EP%253Futm_source%253Dgoogle%2526utm_medium%253Dcpc%2526utm_campaign%253Dasc-int-null-prodfolderdynamic-cpc-pf-google-wwe_int%2526utm_content%253Dprodfolddynamic%2526ds_k%253DDYNAMIC%2BSEARCH%2BADS%2526DCM%253Dyes%2526gclid%253DCjwKCAjwzuqgBhAcEiwAdj5dRvR_WgyvqqhLxMx8zfbFv2a6tg33JIMv01Bn4M1kA4JzW1nDDW7OzhoCRbkQAvD_BwE%2526gclsrc%253Daw.ds")
	(property "Reference" "REF**"
		(at -1.25 -1.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "UQFN-16-1.8x2.6mm_P0.4mm_Texas_RSV0016A"
		(at -1.25 2.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "."
		(at -1.45 -0.75 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at -1.25 3.75 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.25 5 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.25 6.25 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.75 -0.6)
		(size 0.7 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "2" smd roundrect
		(at -0.802 -0.202)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "3" smd roundrect
		(at -0.802 0.2)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "4" smd roundrect
		(at -0.802 0.598)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "5" smd roundrect
		(at -0.6 1.199 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "6" smd roundrect
		(at -0.202 1.199 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "7" smd roundrect
		(at 0.2 1.199 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "8" smd roundrect
		(at 0.598 1.199 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "9" smd roundrect
		(at 0.8 0.598)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "10" smd roundrect
		(at 0.8 0.2)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "11" smd roundrect
		(at 0.8 -0.202)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "12" smd roundrect
		(at 0.8 -0.6)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "13" smd roundrect
		(at 0.598 -1.2 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "14" smd roundrect
		(at 0.2 -1.2 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "15" smd roundrect
		(at -0.202 -1.2 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(pad "16" smd roundrect
		(at -0.6 -1.2 90)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2272727273)
	)
	(embedded_fonts no)
	(model "antmicro_tmux1574rsvr.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
