(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS2034DR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 31.75 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS2034DR"
				(at 31.75 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS2034DR"
				(at 31.75 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2034.pdf?ts=1641906418967&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTPS2034%253FHQS%253DTI-null-null-octopart-df-pf-null-wwe"
				(at 31.75 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power Load Switch, High Side, Active High, 1 Output, 0.033 ohm On State, 5.5 V supp, 3 A, SOIC-8"
				(at 31.75 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS2034DR"
				(at 31.75 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 31.75 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 31.75 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 31.75 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SWITCH, IC, POWER, DRIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS2034DR_1_1"
				(pin passive line
					(at 17.78 -11.43 180)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "In")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "In")
					(number "3")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "En")
					(number "4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{Oc}")
					(number "5")
				)
				(pin power_out line
					(at 17.78 0 180)
					(length 2.54)
					(name "Out")
					(number "6")
				)
				(pin passive line
					(at 17.78 -2.54 180)
					(length 2.54)
					(name "Out")
					(number "7")
				)
				(pin passive line
					(at 17.78 -5.08 180)
					(length 2.54)
					(name "Out")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
