(footprint "Texas_DSBGA-6_1.2x0.8mm_Layout2x3_P0.4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -1.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DSBGA-6_1.2x0.8mm_Layout2x3_P0.4mm"
		(at 0 1.85 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.428 4.277 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.428 5.477 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.428 6.677 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.2 -0.4)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at 0.2 -0.4)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -0.2 0)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at 0.2 0)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -0.2 0.4)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at 0.2 0.4)
		(size 0.25 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_tps22922yfpr.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
