(footprint "Texas_DSBGA-6_1.39x0.9mm_Layout2x3_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "YZP0006")
	(tags "Integrated Circuit")
	(property "Reference" "REF**"
		(at -1.016 -2.032 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DSBGA-6_1.39x0.9mm_Layout"
		(at 2.032 -0.762 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at 2.032 0.508 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at 2.032 1.708 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 2.032 2.908 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -0.25 -0.5 90)
		(size 0.226 0.226)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at 0.25 -0.5 90)
		(size 0.226 0.226)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -0.25 0 90)
		(size 0.226 0.226)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at 0.25 0 90)
		(size 0.226 0.226)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -0.25 0.5 90)
		(size 0.226 0.226)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at 0.25 0.5 90)
		(size 0.226 0.226)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_tps22922yzpr.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
