(footprint "Texas_WSON-14_2x3mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_WSON-14_2x3mm"
		(at 0 2.7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.75 10.85 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.75 12.05 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.75 13.25 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -1.025 -1.2 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "2" smd roundrect
		(at -1.025 -0.8 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "3" smd roundrect
		(at -1.025 -0.4 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "4" smd roundrect
		(at -1.025 0 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "5" smd roundrect
		(at -1.025 0.399 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "6" smd roundrect
		(at -1.025 0.799 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "7" smd roundrect
		(at -1.025 1.199 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "8" smd roundrect
		(at 1.024 1.199 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "9" smd roundrect
		(at 1.024 0.799 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "10" smd roundrect
		(at 1.024 0.399 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "11" smd roundrect
		(at 1.024 0 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "12" smd roundrect
		(at 1.024 -0.4 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "13" smd roundrect
		(at 1.024 -0.8 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "14" smd roundrect
		(at 1.024 -1.2 270)
		(size 0.2 0.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "EP" smd rect
		(at 0 0 270)
		(size 2.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.05)
		(solder_paste_margin -1)
	)
	(embedded_fonts no)
	(model "antmicro_tps22976dpur.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
