(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS22994"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS22994"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS22994"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps22994.pdf?ts=1707303306217"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Quad Channel Load Switch with GPIO and I2C Control"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS22994RUKT"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SWITCH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS22994_1_1"
				(pin power_out line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "VOUT2")
					(number "1")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VIN2")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VBIAS")
					(number "3")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VIN1")
					(number "4")
				)
				(pin power_out line
					(at 19.05 0 180)
					(length 2.54)
					(name "VOUT1")
					(number "5")
				)
				(pin input line
					(at 19.05 -22.86 180)
					(length 2.54)
					(name "ADD1")
					(number "6")
				)
				(pin input line
					(at 19.05 -19.05 180)
					(length 2.54)
					(name "ON4")
					(number "7")
				)
				(pin input line
					(at 19.05 -16.51 180)
					(length 2.54)
					(name "ON3")
					(number "8")
				)
				(pin input line
					(at 19.05 -13.97 180)
					(length 2.54)
					(name "ON2")
					(number "9")
				)
				(pin input line
					(at 19.05 -11.43 180)
					(length 2.54)
					(name "ON1")
					(number "10")
				)
				(pin power_out line
					(at 19.05 -7.62 180)
					(length 2.54)
					(name "VOUT4")
					(number "11")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VIN4")
					(number "12")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VIN3")
					(number "14")
				)
				(pin power_out line
					(at 19.05 -5.08 180)
					(length 2.54)
					(name "VOUT3")
					(number "15")
				)
				(pin input line
					(at 19.05 -25.4 180)
					(length 2.54)
					(name "ADD2")
					(number "16")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "SCL")
					(number "17")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 2.54)
					(name "SDA")
					(number "19")
				)
				(pin input line
					(at 19.05 -27.94 180)
					(length 2.54)
					(name "ADD3")
					(number "20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "EP")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
