(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS2373-3RGW"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS2373-3RGW"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS2373-3RGW"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps2373.pdf?ts=1659968389615&ref_url=https%253A%252F%252Fwww.ti.com%252Fpower-management%252Fpower-over-ethernet-poe%252Fpowered-devices%252Fproducts.html"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Power distribution switch/load driver"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS2373-3RGWR"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SWITCH, IC, POWER, DRIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS2373-3RGW_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DEN")
					(number "2")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "CLSA")
					(number "3")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CLSB")
					(number "6")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 2.54)
					(name "REF")
					(number "7")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "AMPS_CTL")
					(number "8")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 2.54)
					(name "MPS_DUTY")
					(number "9")
				)
				(pin input line
					(at 30.48 -19.05 180)
					(length 2.54)
					(name "APD")
					(number "10")
				)
				(pin power_out line
					(at 30.48 -24.13 180)
					(length 2.54)
					(name "RTN")
					(number "11")
				)
				(pin passive line
					(at 30.48 -24.13 180)
					(length 2.54)
					(hide yes)
					(name "RTN")
					(number "12")
				)
				(pin output line
					(at 30.48 -16.51 180)
					(length 2.54)
					(name "PG")
					(number "13")
				)
				(pin output line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "VC_OUT")
					(number "14")
				)
				(pin input line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "VC_IN")
					(number "15")
				)
				(pin output line
					(at 30.48 -31.75 180)
					(length 2.54)
					(name "UVLO_SEL")
					(number "16")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "TPL")
					(number "17")
				)
				(pin output line
					(at 30.48 0 180)
					(length 2.54)
					(name "TPH")
					(number "18")
				)
				(pin output line
					(at 30.48 -29.21 180)
					(length 2.54)
					(name "~{BT}")
					(number "19")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
