(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS51220A"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 41.91 1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS51220A"
				(at 41.91 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS51220A"
				(at 41.91 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps51220a.pdf?ts=1723633166468"
				(at 41.91 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC/DC converter"
				(at 41.91 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 41.91 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS51220A"
				(at 41.91 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 41.91 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, SWITCHING, VOLTAGE, REGULATOR, DC-DC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS51220A_1_1"
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "V5SW")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RF")
					(number "3")
				)
				(pin input line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "FUNC")
					(number "11")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "12")
				)
				(pin output line
					(at 25.4 0 180)
					(length 2.54)
					(name "VREF2")
					(number "13")
				)
				(pin input line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "TRIP")
					(number "14")
				)
				(pin output line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "VREG3")
					(number "22")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "23")
				)
				(pin power_in line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "GND")
					(number "28")
				)
				(pin output line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "VREG5")
					(number "29")
				)
				(pin power_in line
					(at 25.4 -25.4 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "33")
				)
			)
			(symbol "TPS51220A_2_1"
				(pin power_out line
					(at 25.4 0 180)
					(length 2.54)
					(name "DRVH1")
					(number "1")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "EN1")
					(number "4")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "PGOOD1")
					(number "5")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SKIPSEL1")
					(number "6")
				)
				(pin bidirectional line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "CSP1")
					(number "7")
				)
				(pin input line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "CSN1")
					(number "8")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "VFB1")
					(number "9")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "COMP1")
					(number "10")
				)
				(pin output line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "DRVL1")
					(number "30")
				)
				(pin input line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "VBST1")
					(number "31")
				)
				(pin bidirectional line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "SW1")
					(number "32")
				)
			)
			(symbol "TPS51220A_3_1"
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "COMP2")
					(number "15")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "VFB2")
					(number "16")
				)
				(pin input line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "CSN2")
					(number "17")
				)
				(pin bidirectional line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "CSP2")
					(number "18")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SKIPSEL2")
					(number "19")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "PGOOD2")
					(number "20")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "EN2")
					(number "21")
				)
				(pin power_out line
					(at 25.4 0 180)
					(length 2.54)
					(name "DRVH2")
					(number "24")
				)
				(pin bidirectional line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "SW2")
					(number "25")
				)
				(pin input line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "VBST2")
					(number "26")
				)
				(pin output line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "DRVL2")
					(number "27")
				)
			)
			(embedded_fonts no)
		)
)
