(footprint "Texas_VSON-10-1EP_3x3mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Texas DRC0010J, VSON10 3x3mm Body, 0.5mm Pitch,  http://www.ti.com/lit/ds/symlink/tps63000.pdf")
	(tags "Texas VSON10 3x3mm")
	(property "Reference" "REF**"
		(at 0.02 -2.702 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_VSON-10-1EP_3x3mm_P0.5mm"
		(at -2 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -2 5.549 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2 6.749 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2 7.95 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.25 -1.53)
		(size 0.25 0.34)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at -0.25 1.527)
		(size 0.25 0.34)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0 -0.63)
		(size 1.5 1.06)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0 0.627)
		(size 1.5 1.06)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0.247 -1.53)
		(size 0.25 0.34)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0.247 1.527)
		(size 0.25 0.34)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "1" smd rect
		(at -1.401 -1)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.401 -0.5)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.401 0)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.401 0.497)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.401 0.997)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.398 0.997)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.398 0.497)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.398 0)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.398 -0.5)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.398 -1)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd custom
		(at 0 0)
		(size 1.65 2.4)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.125 -1.1) (xy 0.125 -1.1) (xy 0.125 -1.7) (xy 0.375 -1.7) (xy 0.375 1.7) (xy 0.125 1.7)
					(xy 0.125 1.1) (xy -0.125 1.1) (xy -0.125 1.7) (xy -0.375 1.7) (xy -0.375 -1.7) (xy -0.125 -1.7)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_tps61232drct.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
