(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS62821DLCR"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 31.75 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS62821DLCR"
				(at 31.75 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS62821DLCR"
				(at 31.75 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps62821.pdf?ts=1707379283897&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTPS62821%252Fpart-details%252FTPS62821DLCR"
				(at 31.75 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC/DC converter"
				(at 31.75 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS62821DLCR"
				(at 31.75 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 31.75 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 31.75 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 31.75 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, SWITCHING, VOLTAGE, REGULATOR, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS62821DLCR_1_1"
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "EN")
					(number "1")
				)
				(pin bidirectional line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "FB")
					(number "2")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 2.54)
					(name "AGND")
					(number "3")
				)
				(pin no_connect line
					(at 17.78 -3.81 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin power_in line
					(at 20.32 -11.43 180)
					(length 2.54)
					(name "PGND")
					(number "5")
				)
				(pin bidirectional line
					(at 20.32 0 180)
					(length 2.54)
					(name "SW")
					(number "6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN")
					(number "7")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "PG")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
