(footprint "VQFN-HR-13_2x3mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Based on: https://4donline.ihs.com/images/VipMasterIC/IC/TXII/TXII-S-A0025806545/TXII-S-A0025801067-1.pdf?hkey=61A2E4C270F0397D049F8F05BD4F1054")
	(property "Reference" "REF**"
		(at -1.53 -2.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "VQFN-HR-13_2x3mm"
		(at -1.53 2.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 -0.05 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 0 -0.05 0)
		(layer "F.Fab")
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -1.57 6.48 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -1.53 4.15 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.5 5.34 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 0 -0.05 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at 0 -0.05 0)
		(layer "User.9")
	)
	(pad "1" smd roundrect
		(at -0.95 -0.55 90)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.4)
		(chamfer bottom_right)
	)
	(pad "2" smd roundrect
		(at -0.95 -0.05 90)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "3" smd roundrect
		(at -0.95 0.45 90)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.4)
		(chamfer bottom_left)
	)
	(pad "4" smd roundrect
		(at -0.5 1.3)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.3)
		(chamfer top_left)
	)
	(pad "5" smd roundrect
		(at 0 1.3)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "6" smd roundrect
		(at 0.5 1.3)
		(size 0.25 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.3)
		(chamfer top_right)
	)
	(pad "7" smd roundrect
		(at 0.95 0.45 90)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.4)
		(chamfer top_left)
	)
	(pad "8" smd roundrect
		(at 0.95 -0.05 90)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(pad "9" smd roundrect
		(at 0.95 -0.55 90)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
		(chamfer_ratio 0.4)
		(chamfer top_right)
	)
	(pad "10" smd roundrect
		(at 0.5 -1.52)
		(size 0.245 0.66)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0 -1.57)
		(size 0.25 0.56)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 0 -1.15 90)
		(size 0.4 1.245)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.2)
		(chamfer top_left top_right bottom_left bottom_right)
	)
	(pad "12" smd roundrect
		(at -0.5 -1.525)
		(size 0.25 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 0 -0.05 90)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2)
	)
	(embedded_fonts no)
	(model "antmicro_tps6286a06vbmr.glb"
		(offset
			(xyz -0 0.05 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
