(footprint "VQFN-18_3x3x1mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -2.2 -2.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "VQFN-18_3x3x1mm_P0.5mm"
		(at -2.1 3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -2.296 5 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -2.296 6.2 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.296 7.4 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.45 -0.033)
		(size 0.2 1)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at -0.45 1.205)
		(size 0.2 1)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 0 -1.2045)
		(size 0.2 1)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 0 0.0385)
		(size 0.2 1)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 0.45 -0.033)
		(size 0.2 1)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "" smd roundrect
		(at 0.45 1.205)
		(size 0.2 1)
		(layers "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "1" smd roundrect
		(at -1.4 -1.25 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "1" smd roundrect
		(at -1.24 -1.415 180)
		(size 0.28 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08928571429)
	)
	(pad "2" smd roundrect
		(at -1.4 -0.75 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "3" smd roundrect
		(at -1.4 -0.25 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "4" smd roundrect
		(at -1.4 0.25 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "5" smd roundrect
		(at -1.4 0.75 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "6" smd roundrect
		(at -1.4 1.25 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "6" smd roundrect
		(at -1.24 1.415 180)
		(size 0.28 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08928571429)
	)
	(pad "7" smd roundrect
		(at -0.45 0.586)
		(size 0.2 2.238)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.125)
	)
	(pad "8" smd roundrect
		(at 0 1.355)
		(size 0.2 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "9" smd roundrect
		(at 0.45 0.586)
		(size 0.2 2.238)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.125)
	)
	(pad "10" smd roundrect
		(at 1.24 1.415 180)
		(size 0.28 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08928571429)
	)
	(pad "10" smd roundrect
		(at 1.4 1.25 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "11" smd roundrect
		(at 1.4 0.75 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "12" smd roundrect
		(at 1.4 0.25 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "13" smd roundrect
		(at 1.4 -0.25 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "14" smd roundrect
		(at 1.4 -0.75 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "15" smd roundrect
		(at 1.24 -1.415 180)
		(size 0.28 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.08928571429)
	)
	(pad "15" smd roundrect
		(at 1.4 -1.25 90)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "16" smd roundrect
		(at 0.65 -1.4)
		(size 0.2 0.6096)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(pad "17" smd roundrect
		(at 0 -0.583)
		(size 0.2 2.243)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.125)
	)
	(pad "18" smd roundrect
		(at -0.65 -1.4)
		(size 0.2 0.6096)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.125)
	)
	(embedded_fonts no)
	(model "antmicro_tps65295rjet.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
