(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS65296RJE"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS65296RJE"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS65296RJE"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps65296.pdf"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DC/DC switching voltage regulator"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS65296RJER"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, PMIC, IC, SWITCHING, VOLTAGE, REGULATOR, DC-DC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS65296RJE_1_1"
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "VLDOIN")
					(number "1")
				)
				(pin input line
					(at 27.94 -35.56 180)
					(length 2.54)
					(name "VDDQ")
					(number "2")
				)
				(pin input line
					(at 27.94 -50.8 180)
					(length 2.54)
					(name "AGND")
					(number "3")
				)
				(pin input line
					(at 27.94 -38.1 180)
					(length 2.54)
					(name "VDDQSNS")
					(number "4")
				)
				(pin input line
					(at 27.94 -25.4 180)
					(length 2.54)
					(name "VDD2SNS")
					(number "5")
				)
				(pin input line
					(at 27.94 -43.18 180)
					(length 2.54)
					(name "VDDQREF")
					(number "6")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "PVIN")
					(number "7")
				)
				(pin input line
					(at 27.94 0 180)
					(length 2.54)
					(name "PGOOD")
					(number "8")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "PGND")
					(number "9")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDQEN")
					(number "10")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "VDDEN")
					(number "11")
				)
				(pin input line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "VDD1SNS")
					(number "12")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "VCC_5V")
					(number "13")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "PIN_VDD1")
					(number "14")
				)
				(pin input line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "SW_VDD1")
					(number "15")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 2.54)
					(name "PGND_VDD1")
					(number "16")
				)
				(pin input line
					(at 27.94 -22.86 180)
					(length 2.54)
					(name "SW")
					(number "17")
				)
				(pin input line
					(at 27.94 -15.24 180)
					(length 2.54)
					(name "BST")
					(number "18")
				)
			)
			(embedded_fonts no)
		)
)
