(footprint "Texas_X2QFN-14_2x2mm_P0.4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "RUC (S-PX2QFN-N14)")
	(tags "Integrated Circuit")
	(property "Reference" "REF**"
		(at 0 -1.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_X2QFN-14_2x2mm_P0.4mm"
		(at 0 2.201 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -0.999 4.201 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -0.999 5.4 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -0.999 6.6 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.997 -0.805 90)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.997 -0.405 90)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -0.997 0.003 90)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.997 0.403 90)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -0.997 0.803 90)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -0.204 0.951)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.203 0.951)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 0.995 0.803 90)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.995 0.403 90)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0.995 0.003 90)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.995 -0.405 90)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 0.995 -0.805 90)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 0.203 -0.953)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -0.204 -0.953)
		(size 0.2 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_ts3a4751rucr.glb"
		(offset
			(xyz 0.003 -0.003 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
