(footprint "WQFN-42-1EP_3.5x9mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "WQFN, 42 Pin (http://www.ti.com/lit/ds/symlink/ts3l501e.pdf#page=23), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "WQFN NoLead")
	(property "Reference" "REF**"
		(at -0.875 -5.6 0)
		(layer "F.SilkS")
	)
	(property "Value" "WQFN-42-1EP_3.5x9mm_P0.5mm_EP2.05x7.55mm"
		(at -2.8 6.35 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -2.73 7.82 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -2.73 9.02 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -2.73 10.22 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.56 -2.925)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.56 -1.755)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.56 -0.585)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.56 0.585)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.56 1.755)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.56 2.925)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.56 -2.925)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.56 -1.755)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.56 -0.585)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.56 0.585)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.56 1.755)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.56 2.925)
		(size 0.92 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -1.688 -4)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "2" smd roundrect
		(at -1.688 -3.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "3" smd roundrect
		(at -1.688 -3)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "4" smd roundrect
		(at -1.688 -2.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "5" smd roundrect
		(at -1.688 -2)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "6" smd roundrect
		(at -1.688 -1.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "7" smd roundrect
		(at -1.688 -1)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "8" smd roundrect
		(at -1.688 -0.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "9" smd roundrect
		(at -1.688 0)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "10" smd roundrect
		(at -1.688 0.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "11" smd roundrect
		(at -1.688 1)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "12" smd roundrect
		(at -1.688 1.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "13" smd roundrect
		(at -1.688 2)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "14" smd roundrect
		(at -1.688 2.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "15" smd roundrect
		(at -1.688 3)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "16" smd roundrect
		(at -1.688 3.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "17" smd roundrect
		(at -1.688 4)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "18" smd roundrect
		(at -0.75 4.437)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "19" smd roundrect
		(at -0.25 4.437)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "20" smd roundrect
		(at 0.25 4.437)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "21" smd roundrect
		(at 0.75 4.437)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "22" smd roundrect
		(at 1.687 4)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "23" smd roundrect
		(at 1.687 3.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "24" smd roundrect
		(at 1.687 3)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "25" smd roundrect
		(at 1.687 2.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "26" smd roundrect
		(at 1.687 2)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "27" smd roundrect
		(at 1.687 1.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "28" smd roundrect
		(at 1.687 1)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "29" smd roundrect
		(at 1.687 0.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "30" smd roundrect
		(at 1.687 0)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "31" smd roundrect
		(at 1.687 -0.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "32" smd roundrect
		(at 1.687 -1)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "33" smd roundrect
		(at 1.687 -1.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "34" smd roundrect
		(at 1.687 -2)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "35" smd roundrect
		(at 1.687 -2.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "36" smd roundrect
		(at 1.687 -3)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "37" smd roundrect
		(at 1.687 -3.5)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "38" smd roundrect
		(at 1.687 -4)
		(size 0.875 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "39" smd roundrect
		(at 0.75 -4.438)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "40" smd roundrect
		(at 0.25 -4.438)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "41" smd roundrect
		(at -0.25 -4.438)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "42" smd roundrect
		(at -0.75 -4.438)
		(size 0.25 0.875)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin 0.05)
	)
	(pad "43" thru_hole circle
		(at -0.775 -2.34)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at -0.775 -1.17)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at -0.775 0)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at -0.775 1.17)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at -0.775 2.34)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0 -3.5)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0 -2.34)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0 -1.17)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0 0)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" smd rect
		(at 0 0)
		(size 2.05 7.55)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.05)
	)
	(pad "43" thru_hole circle
		(at 0 1.17)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0 2.34)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0 3.5)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0.775 -2.34)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0.775 -1.17)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0.775 0)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0.775 1.17)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "43" thru_hole circle
		(at 0.775 2.34)
		(size 0.2 0.2)
		(drill 0.2)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_ts3dv642a0ruar.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
