(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TS3DV642A0RUAR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 41.91 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TS3DV642A0RUAR"
				(at 41.91 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TS3DV642A0RUAR"
				(at 41.91 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/scds343d/scds343d.pdf"
				(at 41.91 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "12-Channel 1:2 MUX/DEMUX with 1.8 V Compatible Control and Power-Down Mode"
				(at 41.91 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TS3DV642A0RUAR"
				(at 41.91 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 41.91 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 41.91 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, MUX, SIGNAL, SWITCH"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TS3DV642A0RUAR_0_1")
			(symbol "TS3DV642A0RUAR_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "1")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "EN")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "SCL")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "SDA")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "D0+")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "D0-")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "D1+")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "D1-")
					(number "8")
				)
				(pin no_connect line
					(at 2.54 -58.42 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "D2+")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "D2-")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "D3+")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "D3-")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "HPD")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "CEC")
					(number "15")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SEL1")
					(number "16")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "SEL2")
					(number "17")
				)
				(pin bidirectional line
					(at 29.21 -29.21 180)
					(length 2.54)
					(name "CEC_{A}")
					(number "18")
				)
				(pin bidirectional line
					(at 29.21 -26.67 180)
					(length 2.54)
					(name "HPD_{A}")
					(number "19")
				)
				(pin bidirectional line
					(at 29.21 -64.77 180)
					(length 2.54)
					(name "CEC_{B}")
					(number "20")
				)
				(pin bidirectional line
					(at 29.21 -62.23 180)
					(length 2.54)
					(name "HPD_{B}")
					(number "21")
				)
				(pin bidirectional line
					(at 29.21 -54.61 180)
					(length 2.54)
					(name "D3-_{B}")
					(number "22")
				)
				(pin bidirectional line
					(at 29.21 -52.07 180)
					(length 2.54)
					(name "D3+_{B}")
					(number "23")
				)
				(pin bidirectional line
					(at 29.21 -49.53 180)
					(length 2.54)
					(name "D2-_{B}")
					(number "24")
				)
				(pin bidirectional line
					(at 29.21 -46.99 180)
					(length 2.54)
					(name "D2+_{B}")
					(number "25")
				)
				(pin bidirectional line
					(at 29.21 -44.45 180)
					(length 2.54)
					(name "D1-_{B}")
					(number "26")
				)
				(pin bidirectional line
					(at 29.21 -41.91 180)
					(length 2.54)
					(name "D1+_{B}")
					(number "27")
				)
				(pin bidirectional line
					(at 29.21 -39.37 180)
					(length 2.54)
					(name "D0-_{B}")
					(number "28")
				)
				(pin bidirectional line
					(at 29.21 -36.83 180)
					(length 2.54)
					(name "D0+_{B}")
					(number "29")
				)
				(pin no_connect line
					(at 2.54 -60.96 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "30")
				)
				(pin bidirectional line
					(at 29.21 -19.05 180)
					(length 2.54)
					(name "D3-_{A}")
					(number "31")
				)
				(pin bidirectional line
					(at 29.21 -16.51 180)
					(length 2.54)
					(name "D3+_{A}")
					(number "32")
				)
				(pin bidirectional line
					(at 29.21 -13.97 180)
					(length 2.54)
					(name "D2-_{A}")
					(number "33")
				)
				(pin bidirectional line
					(at 29.21 -11.43 180)
					(length 2.54)
					(name "D2+_{A}")
					(number "34")
				)
				(pin bidirectional line
					(at 29.21 -8.89 180)
					(length 2.54)
					(name "D1-_{A}")
					(number "35")
				)
				(pin bidirectional line
					(at 29.21 -6.35 180)
					(length 2.54)
					(name "D1+_{A}")
					(number "36")
				)
				(pin bidirectional line
					(at 29.21 -3.81 180)
					(length 2.54)
					(name "D0-_{A}")
					(number "37")
				)
				(pin bidirectional line
					(at 29.21 -1.27 180)
					(length 2.54)
					(name "D0+_{A}")
					(number "38")
				)
				(pin bidirectional line
					(at 29.21 -59.69 180)
					(length 2.54)
					(name "SDA_{B}")
					(number "39")
				)
				(pin bidirectional line
					(at 29.21 -57.15 180)
					(length 2.54)
					(name "SCL_{B}")
					(number "40")
				)
				(pin bidirectional line
					(at 29.21 -24.13 180)
					(length 2.54)
					(name "SDA_{A}")
					(number "41")
				)
				(pin bidirectional line
					(at 29.21 -21.59 180)
					(length 2.54)
					(name "SCL_{A}")
					(number "42")
				)
				(pin power_in line
					(at 0 -64.77 0)
					(length 2.54)
					(name "GND")
					(number "43")
				)
			)
			(embedded_fonts no)
		)
)
