(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TS3L500RHUR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TS3L500RHUR"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TS3L500RHUR"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ts3l500.pdf?ts=1663940859045&ref_url=https%253A%252F%252Fwww.google.com%252F"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Logic signal switch/multiplexer/decoder"
				(at 40.64 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TS3L500RHUR"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, SIGNAL, MUX, SWITCH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "RHU56_8P4X2P4"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TS3L500RHUR_1_1"
				(pin power_in line
					(at 0 -67.31 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "A0")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "A1")
					(number "3")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "4")
				)
				(pin no_connect line
					(at 2.54 -59.69 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "A2")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "A3")
					(number "8")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "A4")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "A5")
					(number "12")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "A6")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "A7")
					(number "15")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "16")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SEL")
					(number "17")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 2.54)
					(name "LED0")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 2.54)
					(name "LED1")
					(number "20")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin bidirectional line
					(at 26.67 -25.4 180)
					(length 2.54)
					(name "0LED1")
					(number "22")
				)
				(pin bidirectional line
					(at 26.67 -27.94 180)
					(length 2.54)
					(name "1LED1")
					(number "23")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "24")
				)
				(pin bidirectional line
					(at 26.67 -62.23 180)
					(length 2.54)
					(name "0LED2")
					(number "25")
				)
				(pin bidirectional line
					(at 26.67 -64.77 180)
					(length 2.54)
					(name "1LED2")
					(number "26")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "27")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "28")
				)
				(pin bidirectional line
					(at 26.67 -57.15 180)
					(length 2.54)
					(name "7B2")
					(number "29")
				)
				(pin bidirectional line
					(at 26.67 -54.61 180)
					(length 2.54)
					(name "6B2")
					(number "30")
				)
				(pin bidirectional line
					(at 26.67 -21.59 180)
					(length 2.54)
					(name "7B1")
					(number "31")
				)
				(pin bidirectional line
					(at 26.67 -19.05 180)
					(length 2.54)
					(name "6B1")
					(number "32")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "33")
				)
				(pin bidirectional line
					(at 26.67 -50.8 180)
					(length 2.54)
					(name "5B2")
					(number "34")
				)
				(pin bidirectional line
					(at 26.67 -48.26 180)
					(length 2.54)
					(name "4B2")
					(number "35")
				)
				(pin bidirectional line
					(at 26.67 -15.24 180)
					(length 2.54)
					(name "5B1")
					(number "36")
				)
				(pin bidirectional line
					(at 26.67 -12.7 180)
					(length 2.54)
					(name "4B1")
					(number "37")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "38")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "39")
				)
				(pin bidirectional line
					(at 26.67 -44.45 180)
					(length 2.54)
					(name "3B2")
					(number "40")
				)
				(pin bidirectional line
					(at 26.67 -41.91 180)
					(length 2.54)
					(name "2B2")
					(number "41")
				)
				(pin bidirectional line
					(at 26.67 -8.89 180)
					(length 2.54)
					(name "3B1")
					(number "42")
				)
				(pin bidirectional line
					(at 26.67 -6.35 180)
					(length 2.54)
					(name "2B1")
					(number "43")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "44")
				)
				(pin bidirectional line
					(at 26.67 -38.1 180)
					(length 2.54)
					(name "1B2")
					(number "45")
				)
				(pin bidirectional line
					(at 26.67 -35.56 180)
					(length 2.54)
					(name "0B2")
					(number "46")
				)
				(pin bidirectional line
					(at 26.67 -2.54 180)
					(length 2.54)
					(name "1B1")
					(number "47")
				)
				(pin bidirectional line
					(at 26.67 0 180)
					(length 2.54)
					(name "0B1")
					(number "48")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "49")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "50")
				)
				(pin bidirectional line
					(at 26.67 -67.31 180)
					(length 2.54)
					(name "2LED2")
					(number "51")
				)
				(pin bidirectional line
					(at 26.67 -30.48 180)
					(length 2.54)
					(name "2LED1")
					(number "52")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "53")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 2.54)
					(name "LED2")
					(number "54")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "55")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "56")
				)
				(pin unspecified line
					(at 0 -64.77 0)
					(length 2.54)
					(name "EP")
					(number "57")
				)
			)
			(embedded_fonts no)
		)
)
