(footprint "Texas_DSBGA-36_2.42x2.42mm_Layout6x6_P0.4x0.4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(tags "Integrated Circuit")
	(property "Reference" "REF**"
		(at 0 -1.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DSBGA-36_2.42x2.42mm_Layout6x6_P0.4x0.4mm"
		(at 0 2.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -1.31 4.6 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.31 5.8 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -1.31 7 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -1 -1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -0.6 -1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -0.2 -1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at 0.2 -1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at 0.6 -1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at 1 -1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -1 -0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -0.6 -0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -0.2 -0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at 0.2 -0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at 0.6 -0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at 1 -0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -1 -0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -0.6 -0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -0.2 -0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at 0.2 -0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at 0.6 -0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at 1 -0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -1 0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -0.6 0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -0.2 0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at 0.2 0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at 0.6 0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at 1 0.2 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -1 0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -0.6 0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -0.2 0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at 0.2 0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at 0.6 0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at 1 0.6 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -1 1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -0.6 1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -0.2 1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at 0.2 1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at 0.6 1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F6" smd circle
		(at 1 1 90)
		(size 0.23 0.23)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_ts5mp645nyfpr.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
