(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TS5MP645NYFPR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 41.91 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TS5MP645NYFPR"
				(at 41.91 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TS5MP645NYFPR"
				(at 41.91 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/TS5MP645"
				(at 41.91 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "1.5-pF, 5-V, 2:1 (SPDT), 10-channel MIPI analog switch with powered-off protection & 1.8-V logic"
				(at 41.91 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TS5MP645NYFPR"
				(at 41.91 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 41.91 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 41.91 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, MUX, SIGNAL, SWITCH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TS5MP645NYFPR_0_0"
				(text "HOST"
					(at 10.16 -27.94 900)
				)
				(text "DEVICE A"
					(at 12.7 -12.7 900)
				)
				(text "DEVICE B"
					(at 12.7 -43.18 900)
				)
			)
			(symbol "TS5MP645NYFPR_0_1")
			(symbol "TS5MP645NYFPR_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "A1")
				)
				(pin power_in line
					(at 0 -55.88 0)
					(length 2.54)
					(name "GND")
					(number "A2")
				)
				(pin bidirectional line
					(at 24.13 -19.05 180)
					(length 2.54)
					(name "DA4N")
					(number "A3")
				)
				(pin bidirectional line
					(at 24.13 -16.51 180)
					(length 2.54)
					(name "DA4P")
					(number "A4")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{OE}")
					(number "A5")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SEL")
					(number "A6")
				)
				(pin bidirectional line
					(at 24.13 -49.53 180)
					(length 2.54)
					(name "DB4N")
					(number "B1")
				)
				(pin bidirectional line
					(at 24.13 -46.99 180)
					(length 2.54)
					(name "DB4P")
					(number "B2")
				)
				(pin bidirectional line
					(at 24.13 -13.97 180)
					(length 2.54)
					(name "DA3N")
					(number "B3")
				)
				(pin bidirectional line
					(at 24.13 -11.43 180)
					(length 2.54)
					(name "DA3P")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 2.54)
					(name "D4N")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 2.54)
					(name "D4P")
					(number "B6")
				)
				(pin bidirectional line
					(at 24.13 -44.45 180)
					(length 2.54)
					(name "DB3N")
					(number "C1")
				)
				(pin bidirectional line
					(at 24.13 -41.91 180)
					(length 2.54)
					(name "DB3P")
					(number "C2")
				)
				(pin no_connect line
					(at 2.54 -53.34 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "C3")
				)
				(pin no_connect line
					(at 2.54 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "C4")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 2.54)
					(name "D3N")
					(number "C5")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 2.54)
					(name "D3P")
					(number "C6")
				)
				(pin bidirectional line
					(at 24.13 -39.37 180)
					(length 2.54)
					(name "DB2N")
					(number "D1")
				)
				(pin bidirectional line
					(at 24.13 -36.83 180)
					(length 2.54)
					(name "DB2P")
					(number "D2")
				)
				(pin bidirectional line
					(at 24.13 -8.89 180)
					(length 2.54)
					(name "DA2N")
					(number "D3")
				)
				(pin bidirectional line
					(at 24.13 -6.35 180)
					(length 2.54)
					(name "DA2P")
					(number "D4")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 2.54)
					(name "D2N")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 2.54)
					(name "D2P")
					(number "D6")
				)
				(pin bidirectional line
					(at 24.13 -34.29 180)
					(length 2.54)
					(name "DB1N")
					(number "E1")
				)
				(pin bidirectional line
					(at 24.13 -31.75 180)
					(length 2.54)
					(name "DB1P")
					(number "E2")
				)
				(pin bidirectional line
					(at 24.13 -3.81 180)
					(length 2.54)
					(name "DA1N")
					(number "E3")
				)
				(pin bidirectional line
					(at 24.13 -1.27 180)
					(length 2.54)
					(name "DA1P")
					(number "E4")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "D1N")
					(number "E5")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "D1P")
					(number "E6")
				)
				(pin bidirectional line
					(at 24.13 -54.61 180)
					(length 2.54)
					(name "CLKBN")
					(number "F1")
				)
				(pin bidirectional line
					(at 24.13 -52.07 180)
					(length 2.54)
					(name "CLKBP")
					(number "F2")
				)
				(pin bidirectional line
					(at 24.13 -24.13 180)
					(length 2.54)
					(name "CLKAN")
					(number "F3")
				)
				(pin bidirectional line
					(at 24.13 -21.59 180)
					(length 2.54)
					(name "CLKAP")
					(number "F4")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 2.54)
					(name "CLKN")
					(number "F5")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 2.54)
					(name "CLKP")
					(number "F6")
				)
			)
			(embedded_fonts no)
		)
)
