(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "VSC7511XMY"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "VSC7511XMY"
				(at 50.8 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "VSC7511XMY"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/UNG/ProductDocuments/DataSheets/VSC7511_Data-sheet_DS60001801A.pdf"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "4-Port Layer-2 Gigabit Ethernet Switch"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "VSC7511XMY"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, ETHERNET, IC,  SWITCH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "VSC7511XMY_1_1"
				(pin unspecified line
					(at 0 -54.61 0)
					(length 3.81)
					(name "RESERVED_3")
					(number "3")
				)
				(pin bidirectional line
					(at 35.56 0 180)
					(length 3.81)
					(name "GPIO_0")
					(number "4")
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 3.81)
					(name "GPIO_1")
					(number "5")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 3.81)
					(name "GPIO_2")
					(number "6")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 3.81)
					(name "GPIO_3")
					(number "7")
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 3.81)
					(name "GPIO_4")
					(number "8")
				)
				(pin bidirectional line
					(at 35.56 -12.7 180)
					(length 3.81)
					(name "GPIO_5")
					(number "9")
				)
				(pin bidirectional line
					(at 35.56 -15.24 180)
					(length 3.81)
					(name "GPIO_6")
					(number "10")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 3.81)
					(name "GPIO_7")
					(number "11")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 3.81)
					(name "GPIO_8")
					(number "12")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 3.81)
					(name "GPIO_9")
					(number "13")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 3.81)
					(name "GPIO_10")
					(number "14")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 3.81)
					(name "GPIO_11")
					(number "15")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 3.81)
					(name "GPIO_12")
					(number "16")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 3.81)
					(name "GPIO_13")
					(number "17")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 3.81)
					(name "GPIO_14")
					(number "18")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 3.81)
					(name "GPIO_15")
					(number "19")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 3.81)
					(name "GPIO_16")
					(number "20")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 3.81)
					(name "GPIO_17")
					(number "21")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 3.81)
					(name "GPIO_18")
					(number "25")
				)
				(pin bidirectional line
					(at 35.56 -48.26 180)
					(length 3.81)
					(name "GPIO_19")
					(number "26")
				)
				(pin bidirectional line
					(at 35.56 -50.8 180)
					(length 3.81)
					(name "GPIO_20")
					(number "27")
				)
				(pin bidirectional line
					(at 35.56 -53.34 180)
					(length 3.81)
					(name "GPIO_21")
					(number "28")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 3.81)
					(name "SI_DI")
					(number "29")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 3.81)
					(name "SI_DO")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "SI_NCS0")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "SI_CLK")
					(number "32")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "NRESET")
					(number "33")
				)
				(pin output line
					(at 0 -3.81 0)
					(length 3.81)
					(name "JTAG_TDO")
					(number "34")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 3.81)
					(name "JTAG_NTRST")
					(number "35")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 3.81)
					(name "JTAG_TMS")
					(number "36")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 3.81)
					(name "JTAG_TDI")
					(number "37")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 3.81)
					(name "JTAG_TCK")
					(number "38")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "45")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "53")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "71")
				)
				(pin output line
					(at 0 -26.67 0)
					(length 3.81)
					(name "CLKOUTPLL_N")
					(number "79")
				)
				(pin output line
					(at 0 -24.13 0)
					(length 3.81)
					(name "CLKOUTPLL_P")
					(number "81")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "REFCLK_N")
					(number "82")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 3.81)
					(name "REFCLK_P")
					(number "84")
				)
				(pin unspecified line
					(at 0 -48.26 0)
					(length 3.81)
					(name "SERDES_REXT_0")
					(number "85")
				)
				(pin unspecified line
					(at 0 -50.8 0)
					(length 3.81)
					(name "SERDES_REXT_1")
					(number "86")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "87")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "88")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "89")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "90")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "91")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "94")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "106")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "111")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "113")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "115")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "117")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "121")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "123")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "124")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "125")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "126")
				)
				(pin unspecified line
					(at 0 -41.91 0)
					(length 3.81)
					(name "THERMDA")
					(number "127")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "128")
				)
				(pin unspecified line
					(at 0 -44.45 0)
					(length 3.81)
					(name "THERMDC")
					(number "129")
				)
				(pin no_connect line
					(at 31.75 -55.88 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "171")
				)
			)
			(symbol "VSC7511XMY_2_1"
				(pin unspecified line
					(at 0 -24.13 0)
					(length 3.81)
					(name "RESERVED_1")
					(number "131")
				)
				(pin bidirectional line
					(at 29.21 -17.78 180)
					(length 3.81)
					(name "P0_D3N")
					(number "132")
				)
				(pin unspecified line
					(at 0 -21.59 0)
					(length 3.81)
					(name "RESERVED_0")
					(number "133")
				)
				(pin bidirectional line
					(at 29.21 -15.24 180)
					(length 3.81)
					(name "P0_D3P")
					(number "134")
				)
				(pin bidirectional line
					(at 29.21 -12.7 180)
					(length 3.81)
					(name "P0_D2N")
					(number "135")
				)
				(pin bidirectional line
					(at 29.21 -10.16 180)
					(length 3.81)
					(name "P0_D2P")
					(number "137")
				)
				(pin bidirectional line
					(at 29.21 -7.62 180)
					(length 3.81)
					(name "P0_D1N")
					(number "138")
				)
				(pin bidirectional line
					(at 29.21 -2.54 180)
					(length 3.81)
					(name "P0_D0N")
					(number "141")
				)
				(pin bidirectional line
					(at 29.21 -5.08 180)
					(length 3.81)
					(name "P0_D1P")
					(number "142")
				)
				(pin bidirectional line
					(at 29.21 0 180)
					(length 3.81)
					(name "P0_D0P")
					(number "143")
				)
				(pin bidirectional line
					(at 29.21 -39.37 180)
					(length 3.81)
					(name "P1_D3N")
					(number "144")
				)
				(pin bidirectional line
					(at 29.21 -34.29 180)
					(length 3.81)
					(name "P1_D2N")
					(number "145")
				)
				(pin bidirectional line
					(at 29.21 -36.83 180)
					(length 3.81)
					(name "P1_D3P")
					(number "146")
				)
				(pin bidirectional line
					(at 29.21 -31.75 180)
					(length 3.81)
					(name "P1_D2P")
					(number "147")
				)
				(pin bidirectional line
					(at 29.21 -29.21 180)
					(length 3.81)
					(name "P1_D1N")
					(number "148")
				)
				(pin bidirectional line
					(at 29.21 -24.13 180)
					(length 3.81)
					(name "P1_D0N")
					(number "149")
				)
				(pin bidirectional line
					(at 29.21 -26.67 180)
					(length 3.81)
					(name "P1_D1P")
					(number "150")
				)
				(pin bidirectional line
					(at 29.21 -21.59 180)
					(length 3.81)
					(name "P1_D0P")
					(number "151")
				)
				(pin unspecified line
					(at 0 -2.54 0)
					(length 3.81)
					(name "REF_FILT")
					(number "152")
				)
				(pin unspecified line
					(at 0 0 0)
					(length 3.81)
					(name "REF_REXT")
					(number "153")
				)
				(pin bidirectional line
					(at 29.21 -60.96 180)
					(length 3.81)
					(name "P2_D3N")
					(number "154")
				)
				(pin bidirectional line
					(at 29.21 -55.88 180)
					(length 3.81)
					(name "P2_D2N")
					(number "155")
				)
				(pin bidirectional line
					(at 29.21 -58.42 180)
					(length 3.81)
					(name "P2_D3P")
					(number "156")
				)
				(pin bidirectional line
					(at 29.21 -53.34 180)
					(length 3.81)
					(name "P2_D2P")
					(number "157")
				)
				(pin bidirectional line
					(at 29.21 -50.8 180)
					(length 3.81)
					(name "P2_D1N")
					(number "158")
				)
				(pin bidirectional line
					(at 29.21 -45.72 180)
					(length 3.81)
					(name "P2_D0N")
					(number "159")
				)
				(pin bidirectional line
					(at 29.21 -48.26 180)
					(length 3.81)
					(name "P2_D1P")
					(number "160")
				)
				(pin bidirectional line
					(at 29.21 -43.18 180)
					(length 3.81)
					(name "P2_D0P")
					(number "161")
				)
				(pin bidirectional line
					(at 29.21 -82.55 180)
					(length 3.81)
					(name "P3_D3N")
					(number "162")
				)
				(pin bidirectional line
					(at 29.21 -77.47 180)
					(length 3.81)
					(name "P3_D2N")
					(number "163")
				)
				(pin bidirectional line
					(at 29.21 -80.01 180)
					(length 3.81)
					(name "P3_D3P")
					(number "164")
				)
				(pin bidirectional line
					(at 29.21 -74.93 180)
					(length 3.81)
					(name "P3_D2P")
					(number "165")
				)
				(pin bidirectional line
					(at 29.21 -72.39 180)
					(length 3.81)
					(name "P3_D1N")
					(number "167")
				)
				(pin bidirectional line
					(at 29.21 -69.85 180)
					(length 3.81)
					(name "P3_D1P")
					(number "169")
				)
				(pin bidirectional line
					(at 29.21 -67.31 180)
					(length 3.81)
					(name "P3_D0N")
					(number "170")
				)
				(pin bidirectional line
					(at 29.21 -64.77 180)
					(length 3.81)
					(name "P3_D0P")
					(number "172")
				)
			)
			(symbol "VSC7511XMY_3_1"
				(pin output line
					(at 0 -2.54 0)
					(length 3.81)
					(name "S4_TXN")
					(number "44")
				)
				(pin output line
					(at 0 0 0)
					(length 3.81)
					(name "S4_TXP")
					(number "46")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 3.81)
					(name "S4_RXN")
					(number "49")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 3.81)
					(name "S4_RXP")
					(number "51")
				)
				(pin output line
					(at 0 -16.51 0)
					(length 3.81)
					(name "S5_TXN")
					(number "52")
				)
				(pin output line
					(at 0 -13.97 0)
					(length 3.81)
					(name "S5_TXP")
					(number "54")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "S5_RXN")
					(number "55")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "S5_RXP")
					(number "57")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 3.81)
					(name "S6_TXN")
					(number "60")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 3.81)
					(name "S6_TXP")
					(number "62")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 3.81)
					(name "S6_RXN")
					(number "64")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 3.81)
					(name "S6_RXP")
					(number "66")
				)
				(pin output line
					(at 0 -44.45 0)
					(length 3.81)
					(name "S7_TXN")
					(number "67")
				)
				(pin output line
					(at 0 -41.91 0)
					(length 3.81)
					(name "S7_TXP")
					(number "69")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 3.81)
					(name "S7_RXN")
					(number "70")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 3.81)
					(name "S7_RXP")
					(number "72")
				)
				(pin output line
					(at 0 -58.42 0)
					(length 3.81)
					(name "S8_TXN")
					(number "73")
				)
				(pin output line
					(at 0 -55.88 0)
					(length 3.81)
					(name "S8_TXP")
					(number "75")
				)
				(pin input line
					(at 0 -64.77 0)
					(length 3.81)
					(name "S8_RXN")
					(number "76")
				)
				(pin input line
					(at 0 -62.23 0)
					(length 3.81)
					(name "S8_RXP")
					(number "78")
				)
			)
			(symbol "VSC7511XMY_4_1"
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDD")
					(number "1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDD_IO")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "22")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "23")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "24")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "39")
				)
				(pin power_in line
					(at 24.13 0 180)
					(length 3.81)
					(name "VDDA")
					(number "40")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VDDA")
					(number "41")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VDDA")
					(number "42")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "43")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "47")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VDDA")
					(number "48")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD_VS")
					(number "50")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD_VS")
					(number "56")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VDDA")
					(number "58")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "59")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "61")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD_VS")
					(number "63")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VDDA")
					(number "65")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "VDD_VS")
					(number "68")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDD_VS")
					(number "74")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VDDA")
					(number "77")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "80")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "83")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "92")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "93")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "95")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "96")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "97")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "98")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "99")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "100")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "101")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "102")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "103")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "104")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "105")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "107")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "108")
				)
				(pin power_in line
					(at 24.13 -8.89 180)
					(length 3.81)
					(name "VSS")
					(number "109")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "110")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "112")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "114")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "116")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "118")
				)
				(pin passive line
					(at 24.13 -8.89 180)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "119")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "120")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "122")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "130")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD")
					(number "136")
				)
				(pin passive line
					(at 24.13 -5.08 180)
					(length 3.81)
					(hide yes)
					(name "VDD_AL")
					(number "139")
				)
				(pin power_in line
					(at 24.13 -2.54 180)
					(length 3.81)
					(name "VDD_AH")
					(number "140")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VDD_AH")
					(number "166")
				)
				(pin power_in line
					(at 24.13 -5.08 180)
					(length 3.81)
					(name "VDD_AL")
					(number "168")
				)
				(pin power_in line
					(at 24.13 -11.43 180)
					(length 3.81)
					(name "EPAD")
					(number "173")
				)
			)
			(embedded_fonts no)
		)
)
