(footprint "JUMPSM3P"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2 SMD Pads for Bound by Solder Drop - Equivalent Size 0805 - Gap 0.5mm")
	(property "Reference" "REF**"
		(at 0.00004 -1.704 0)
		(layer "F.SilkS")
	)
	(property "Value" "JUMPSM3P"
		(at 0.00004 1.704 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard allow_soldermask_bridges)
	(net_tie_pad_groups "1,2,3")
	(pad "1" smd rect
		(at -1.9 0)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.15)
	)
	(pad "1" smd custom
		(at -1.43096 0.954)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy -0.12559 0) (xy -0.36823 -0.06501) (xy -0.58577 -0.19061) (xy -0.76339 -0.36823) (xy -0.88899 -0.58577)
					(xy -0.954 -0.8284) (xy -0.954 -1.0796) (xy -0.88899 -1.32223) (xy -0.76339 -1.53977) (xy -0.58577 -1.71739)
					(xy -0.36823 -1.84299) (xy -0.12559 -1.908) (xy 0 -1.908) (xy 0.477 -1.908) (xy 0.50863 -1.908)
					(xy 0.56707 -1.88379) (xy 0.6118 -1.83907) (xy 0.636 -1.78063) (xy 0.636 -1.749) (xy 0.636 -1.59)
					(xy 0.636 -1.55837) (xy 0.6118 -1.49993) (xy 0.56707 -1.45521) (xy 0.50863 -1.431) (xy 0.477 -1.431)
					(xy 0.318 -1.431) (xy 0.25597 -1.42489) (xy 0.14133 -1.37741) (xy 0.0536 -1.28967) (xy 0.00611 -1.17504)
					(xy 0 -1.113) (xy 0 -0.795) (xy 0.00611 -0.73296) (xy 0.0536 -0.61833) (xy 0.14133 -0.53059) (xy 0.25597 -0.48311)
					(xy 0.318 -0.477) (xy 0.477 -0.477) (xy 0.50863 -0.477) (xy 0.56707 -0.45279) (xy 0.6118 -0.40807)
					(xy 0.636 -0.34963) (xy 0.636 -0.318) (xy 0.636 -0.159) (xy 0.636 -0.12737) (xy 0.6118 -0.06893)
					(xy 0.56707 -0.02421) (xy 0.50863 0) (xy 0.477 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at -0.47696 0.795)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 -0.318) (xy -0.00305 -0.34902) (xy -0.02679 -0.40634) (xy -0.07066 -0.4502) (xy -0.12798 -0.47395)
					(xy -0.159 -0.477) (xy -0.477 -0.477) (xy -0.50862 -0.477) (xy -0.56706 -0.50121) (xy -0.61179 -0.54593)
					(xy -0.636 -0.60438) (xy -0.63599 -0.636) (xy -0.636 -0.636) (xy -0.63599 -0.954) (xy -0.636 -0.98562)
					(xy -0.61179 -1.04407) (xy -0.56706 -1.08879) (xy -0.50862 -1.113) (xy -0.477 -1.113) (xy -0.159 -1.113)
					(xy -0.12798 -1.11605) (xy -0.07066 -1.1398) (xy -0.02679 -1.18366) (xy -0.00305 -1.24098) (xy 0 -1.272)
					(xy 0.00001 -1.59) (xy 0 -1.62163) (xy 0.02421 -1.68007) (xy 0.06894 -1.72479) (xy 0.12738 -1.749)
					(xy 0.159 -1.749) (xy 0.795 -1.749) (xy 0.82663 -1.749) (xy 0.88507 -1.7248) (xy 0.9298 -1.68007)
					(xy 0.954 -1.62163) (xy 0.954 -1.59) (xy 0.954 -1.272) (xy 0.95706 -1.24098) (xy 0.9808 -1.18366)
					(xy 1.02467 -1.1398) (xy 1.08198 -1.11605) (xy 1.113 -1.113) (xy 1.431 -1.113) (xy 1.46263 -1.113)
					(xy 1.52107 -1.08879) (xy 1.5658 -1.04407) (xy 1.59 -0.98563) (xy 1.59 -0.954) (xy 1.59 -0.636)
					(xy 1.59 -0.60437) (xy 1.5658 -0.54593) (xy 1.52107 -0.50121) (xy 1.46263 -0.477) (xy 1.431 -0.477)
					(xy 1.113 -0.477) (xy 1.08198 -0.47395) (xy 1.02467 -0.4502) (xy 0.9808 -0.40634) (xy 0.95706 -0.34902)
					(xy 0.954 -0.318) (xy 0.954 0) (xy 0.954 0.03163) (xy 0.9298 0.09007) (xy 0.88507 0.1348) (xy 0.82663 0.159)
					(xy 0.795 0.159) (xy 0.159 0.159) (xy 0.12738 0.159) (xy 0.06894 0.13479) (xy 0.02421 0.09007)
					(xy 0 0.03163) (xy 0.00001 0)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd rect
		(at 0 0)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.15)
	)
	(pad "3" smd custom
		(at 0.79504 0.795)
		(size 0.000001 0.000001)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0 -0.159) (xy 0 -0.19063) (xy 0.02421 -0.24907) (xy 0.06894 -0.29379) (xy 0.12738 -0.318)
					(xy 0.159 -0.318) (xy 0.318 -0.318) (xy 0.38004 -0.32411) (xy 0.49467 -0.37159) (xy 0.58241 -0.45933)
					(xy 0.62989 -0.57396) (xy 0.636 -0.636) (xy 0.636 -0.954) (xy 0.62989 -1.01604) (xy 0.58241 -1.13067)
					(xy 0.49467 -1.21841) (xy 0.38004 -1.26589) (xy 0.318 -1.272) (xy 0.159 -1.272) (xy 0.12738 -1.272)
					(xy 0.06894 -1.29621) (xy 0.02421 -1.34093) (xy 0 -1.39937) (xy 0 -1.431) (xy 0 -1.59) (xy 0 -1.62163)
					(xy 0.02421 -1.68007) (xy 0.06894 -1.72479) (xy 0.12738 -1.749) (xy 0.159 -1.749) (xy 0.636 -1.749)
					(xy 0.7616 -1.749) (xy 1.00423 -1.68399) (xy 1.22177 -1.55839) (xy 1.39939 -1.38077) (xy 1.52499 -1.16323)
					(xy 1.59001 -0.9206) (xy 1.59001 -0.6694) (xy 1.52499 -0.42677) (xy 1.39939 -0.20923) (xy 1.22177 -0.03161)
					(xy 1.00423 0.09399) (xy 0.7616 0.159) (xy 0.636 0.159) (xy 0.159 0.159) (xy 0.12738 0.159) (xy 0.06894 0.13479)
					(xy 0.02421 0.09007) (xy 0 0.03163)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd rect
		(at 1.9 0)
		(size 0.3 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.15)
	)
	(embedded_fonts no)
)
