(footprint "JUMPSMD0805_G50"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2 SMD Pads for Bound by Solder Drop - Equivalent Size 0805 - Gap 0.5mm")
	(property "Reference" "REF**"
		(at 0 -1.527 0)
		(layer "F.SilkS")
	)
	(property "Value" "JUMPSMD0805_G50"
		(at 0 1.527 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" smd rect
		(at -1.1875 0)
		(size 0.475 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.225)
	)
	(pad "1" smd rect
		(at -0.6 0)
		(size 0.7 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.35)
	)
	(pad "1" smd custom
		(at -0.25 -0.7)
		(size 0.000001 0.000001)
		(layers "F.Cu")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy -0.7 0) (xy -1.175 0.475) (xy -1.175 0.925) (xy -0.7 1.4) (xy 0 1.4)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 0.25 0.7)
		(size 0.000001 0.000001)
		(layers "F.Cu")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0 0) (xy 0.7 0) (xy 1.175 -0.475) (xy 1.175 -0.925) (xy 0.7 -1.4) (xy 0 -1.4)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd rect
		(at 0.6 0)
		(size 0.7 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.35)
	)
	(pad "2" smd rect
		(at 1.1875 0)
		(size 0.475 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.225)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.05 -0.7) (xy 0.05 -0.7) (xy 0.05 0.7) (xy -0.05 0.7)
			)
		)
	)
	(embedded_fonts no)
)
