(footprint "PB_APEM_TP32P0080"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SPDT Momentary Push-Button Switch - Straight PCB - APEM TP Serie")
	(property "Reference" "REF**"
		(at 0 -3.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_APEM_TP32P0080"
		(at 0 3.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "3"
		(at 2.921 -1.0205 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -3.302 -1.0205 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at 2.92049 -1.02101 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "1"
		(at -3.30251 -1.02101 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -2.54 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 0 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 2.54 0)
		(size 1.8 1.8)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
