(footprint "PB_C&K_8125SH9CBE"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SPDT Snap-acting Momentary Pusbutton Switch, Contact Rating 0.4VA 20V, 8020 Series")
	(property "Reference" "REF**"
		(at 0.02484 -7.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_C&K_8125SH9CBE"
		(at 0.02484 7.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "3"
		(at -4.5 5.3225 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at -4.5 0.6225 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -4.3 -4.0775 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at -4.3 -4.0775 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at -4.5 5.3225 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at -4.5 0.6225 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(pad "1" thru_hole circle
		(at 0 -4.699)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 0 0)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 0 4.699)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
