(footprint "PB_C&K_8221SHCGE"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "DPDT Snap-acting Momentary Pushbutton Switch, Contact Rating 1A 120V, 8020 Series")
	(property "Reference" "REF**"
		(at -0.00016 -7.15 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_C&K_8221SHCGE"
		(at -0.00016 7.15 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "5"
		(at -7 0.4225 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at 6.2 5.4338 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at -7 -4.4511 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "6"
		(at -7 5.4338 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "2"
		(at 6.2 0.4225 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at 6.3 -4.4775 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "1"
		(at 6.3 -4.4775 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "2"
		(at 6.2 0.4225 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "5"
		(at -7 0.4225 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "4"
		(at -7 -4.4511 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "3"
		(at 6.2 5.4338 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "6"
		(at -7 5.4338 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 2.41484 -4.92)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 2.41484 0)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 2.41484 4.92)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -2.41516 -4.92)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at -2.41516 0)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "6" thru_hole circle
		(at -2.41516 4.92)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
