(footprint "PB_C&K_E112SD1AV2BE"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SPDT Toggle Switch - Vertical Right Angled PCB Mounting, Unthreaded Bushing, C&K E010 Series")
	(property "Reference" "REF**"
		(at -11.78251 -4.39 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_C&K_E112SD1AV2BE"
		(at -11.78251 4.39 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" thru_hole circle
		(at -3.81 0 270)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 0 0 270)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 3.81 0 270)
		(size 2.5 2.5)
		(drill 1.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at -16.51001 -2.54)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "7" thru_hole circle
		(at -16.51001 2.54)
		(size 2.3 2.3)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
