(footprint "PB_C&K_KSC321J"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 6.2x6.2mm, Surface Mount Sealed Tact Momentary Pushbutton Switch, C&K KSC3 Series")
	(property "Reference" "REF**"
		(at 0 -4.125 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_C&K_KSC321J"
		(at 0 4.125 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -2.9 -2)
		(size 2.8 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 2.9 -2)
		(size 2.8 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.9 2)
		(size 2.8 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 2.9 2)
		(size 2.8 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
