(footprint "PB_MEC_NAVIKITTH30WL"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Navigation Switch Navimec, 4 x 1ZB Keycaps on 3A Switches And 1 x 1ZC on 3F Switches, Blue Color")
	(property "Reference" "REF**"
		(at 0 -18.30001 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_MEC_NAVIKITTH30WL"
		(at 0 18.30001 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "OK"
		(at -2.05478 1.55614 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "D"
		(at 0.125 11.9275 180)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "L"
		(at -11.9275 0.125 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "U"
		(at -0.125 -11.9275 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "R"
		(at 11.9275 -0.125 270)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "4"
		(at 3.37196 3.0975 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at -14.48251 4.24804 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at -3.37195 14.48251 180)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at 4.24805 9.40251 180)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at -9.40251 -3.37196 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at -4.24804 -1.9825 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at 9.40251 -4.24805 270)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at -4.24804 -9.40251 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at 9.40251 3.37195 270)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at 14.48251 3.37195 270)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at -9.40251 4.24804 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at 3.37196 -14.48251 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at 14.48251 -4.24805 270)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at -4.24804 -14.48251 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at 3.37196 -9.40251 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at -3.37195 9.40251 180)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at 3.37196 -1.9825 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at 4.24805 14.48251 180)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "3"
		(at -4.24804 3.0975 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at -14.48251 -3.37196 90)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "OK"
		(at -2.05478 1.55614 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "C1" thru_hole circle
		(at -5.08 -3.81)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "C2" thru_hole circle
		(at 5.08 -3.81)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "C3" thru_hole circle
		(at -5.08 3.81)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "C4" thru_hole circle
		(at 5.08 3.81)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "D1" thru_hole circle
		(at 5.08 16.31001)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "D2" thru_hole circle
		(at -5.08 16.31001)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "D3" thru_hole circle
		(at 5.08 8.69001)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "D4" thru_hole circle
		(at -5.08 8.69001)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "L1" thru_hole circle
		(at -16.31001 5.08 90)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "L2" thru_hole circle
		(at -16.31001 -5.08 90)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "L3" thru_hole circle
		(at -8.69001 5.08 90)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "L4" thru_hole circle
		(at -8.69001 -5.08 90)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "R1" thru_hole circle
		(at 16.31001 -5.08 90)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "R2" thru_hole circle
		(at 16.31001 5.08 90)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "R3" thru_hole circle
		(at 8.69001 -5.08 90)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "R4" thru_hole circle
		(at 8.69001 5.08 90)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "U1" thru_hole circle
		(at -5.08 -16.31001)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "U2" thru_hole circle
		(at 5.08 -16.31001)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "U3" thru_hole circle
		(at -5.08 -8.69001)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "U4" thru_hole circle
		(at 5.08 -8.69001)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
