(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "PB_MEC_NAVIKITTH30WL"
  		(pin_numbers
  			(hide yes)
  		)
  		(pin_names
  			(offset 1.27)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "PB"
  			(at 12.7 1.27 0)
  		)
  		(property "Value" "${FAMILY}"
  			(at 12.7 -39.37 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "4 pcs. 1ZB Keycaps on 3A Switches And 1 pc. of 1ZC on 3F Switches, MEC NAVIMEC"
  			(at 0 0 0)
  		)
  		(symbol "PB_MEC_NAVIKITTH30WL_1_0"
  			(text "L"
  				(at 12.192 -7.366 0)
  			)
  			(text "OK"
  				(at 16.51 -7.366 0)
  			)
  			(text "U"
  				(at 17.018 -2.286 0)
  			)
  			(text "D"
  				(at 17.272 -12.446 0)
  			)
  			(text "R"
  				(at 22.098 -7.366 0)
  			)
  			(pin bidirectional line
  				(at -5.08 -2.54 0)
  				(length 5.08)
  				(name "L1")
  				(number "L1")
  			)
  			(pin bidirectional line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "L2")
  				(number "L2")
  			)
  			(pin bidirectional line
  				(at -5.08 -7.62 0)
  				(length 5.08)
  				(name "L3")
  				(number "L3")
  			)
  			(pin bidirectional line
  				(at -5.08 -10.16 0)
  				(length 5.08)
  				(name "L4")
  				(number "L4")
  			)
  			(pin bidirectional line
  				(at -5.08 -15.24 0)
  				(length 5.08)
  				(name "R1")
  				(number "R1")
  			)
  			(pin bidirectional line
  				(at -5.08 -17.78 0)
  				(length 5.08)
  				(name "R2")
  				(number "R2")
  			)
  			(pin bidirectional line
  				(at -5.08 -20.32 0)
  				(length 5.08)
  				(name "R3")
  				(number "R3")
  			)
  			(pin bidirectional line
  				(at -5.08 -22.86 0)
  				(length 5.08)
  				(name "R4")
  				(number "R4")
  			)
  			(pin bidirectional line
  				(at -5.08 -27.94 0)
  				(length 5.08)
  				(name "C1")
  				(number "C1")
  			)
  			(pin bidirectional line
  				(at -5.08 -30.48 0)
  				(length 5.08)
  				(name "C2")
  				(number "C2")
  			)
  			(pin bidirectional line
  				(at -5.08 -33.02 0)
  				(length 5.08)
  				(name "C3")
  				(number "C3")
  			)
  			(pin bidirectional line
  				(at -5.08 -35.56 0)
  				(length 5.08)
  				(name "C4")
  				(number "C4")
  			)
  			(pin bidirectional line
  				(at 30.48 -15.24 180)
  				(length 5.08)
  				(name "U1")
  				(number "U1")
  			)
  			(pin bidirectional line
  				(at 30.48 -17.78 180)
  				(length 5.08)
  				(name "U2")
  				(number "U2")
  			)
  			(pin bidirectional line
  				(at 30.48 -20.32 180)
  				(length 5.08)
  				(name "U3")
  				(number "U3")
  			)
  			(pin bidirectional line
  				(at 30.48 -22.86 180)
  				(length 5.08)
  				(name "U4")
  				(number "U4")
  			)
  			(pin bidirectional line
  				(at 30.48 -27.94 180)
  				(length 5.08)
  				(name "D1")
  				(number "D1")
  			)
  			(pin bidirectional line
  				(at 30.48 -30.48 180)
  				(length 5.08)
  				(name "D2")
  				(number "D2")
  			)
  			(pin bidirectional line
  				(at 30.48 -33.02 180)
  				(length 5.08)
  				(name "D3")
  				(number "D3")
  			)
  			(pin bidirectional line
  				(at 30.48 -35.56 180)
  				(length 5.08)
  				(name "D4")
  				(number "D4")
  			)
  		)
  		(embedded_fonts no)
  	)
)
