(footprint "PB_MULTIMEC_5GTH935+1ZCS06118"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 10.1x10.1mm, Pushbutton Switch Round Diam 14.3mm, MULTIMEC 5GTH935+1ZCS")
	(property "Reference" "REF**"
		(at 0 -8.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_MULTIMEC_5GTH935+1ZCS06118"
		(at 0 8.2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "OK"
		(at -2.05478 1.55614 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "3"
		(at -4.24804 3.0975 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "4"
		(at 3.37196 3.0975 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "1"
		(at -4.24804 -1.9825 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "2"
		(at 3.37196 -1.9825 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(fp_text user "OK"
		(at -2.05478 1.55614 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at -5.08 -3.81)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 5.08 -3.81)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at -5.08 3.81)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at 5.08 3.81)
		(size 1.6 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
