(footprint "PB_SCHNEIDER_ZBE701"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Contact Block SPST NO, To be used with ZBZ01x Socket Adaptor")
	(property "Reference" "REF**"
		(at -0.000165 -9.65827 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_SCHNEIDER_ZBE701"
		(at -0.000165 9.65827 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(pad "1" smd circle
		(at -0.00016 -6.35)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.25)
		(thermal_bridge_angle 90)
	)
	(pad "2" smd circle
		(at -0.00016 6.35)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.25)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
