(footprint "PB_TYCO_FSM4JSMA"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 6mm x 6mm, Surface Mount Tactile Switches, TYCO FSMJSMA Series")
	(property "Reference" "REF**"
		(at 0 -6.575 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_TYCO_FSM4JSMA"
		(at 0 6.575 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -2.25 -4.55 90)
		(size 2.1 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.25 4.55 90)
		(size 2.1 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 2.25 -4.55 90)
		(size 2.1 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 2.25 4.55 90)
		(size 2.1 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
