(footprint "PB_TYCO_FSMSM"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body 3.5x6.0mm, Pushbutton Switch,  TYCO FSMSM Serie")
	(property "Reference" "REF**"
		(at 0 -2.725 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_TYCO_FSMSM"
		(at 0 2.725 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -4.65 0)
		(size 2.1 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 4.65 0)
		(size 2.1 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
