(footprint "PB_WURTH_435451019820"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Body L 4.6mm x W 2.8mm x H 1.9mm - Tactil Switch")
	(property "Reference" "REF**"
		(at 0 -2.375 0)
		(layer "F.SilkS")
	)
	(property "Value" "PB_WURTH_435451019820"
		(at 0 2.675 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "1" smd rect
		(at -2.05 0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.05 -0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 2.05 -0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 2.05 0.8)
		(size 0.9 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 0 1.425)
		(size 1.7 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
