(footprint "SW_ALPS_EC11B15242AE"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Encoder, Horizontal With Push-on Switch, ALPS EC11 Series")
	(property "Reference" "REF**"
		(at 0 -4.05 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_ALPS_EC11B15242AE"
		(at 0 24.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "A"
		(at -2.8 1.991875 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "B"
		(at 2.3 1.991875 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "C"
		(at -0.3 1.991875 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(pad "1" thru_hole circle
		(at -2.5 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "2" thru_hole circle
		(at 2.5 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "3" thru_hole circle
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "4" thru_hole circle
		(at -2.5 -2.5)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "5" thru_hole circle
		(at 2.5 -2.5)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "P1" thru_hole circle
		(at -5.85 -1.2)
		(size 3.5 3.5)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "P2" thru_hole circle
		(at 5.85 -1.2)
		(size 3.5 3.5)
		(drill 2.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
