(kicad_symbol_lib (version 20211014) (generator partreel-import)
  (symbol "SW_ALPS_SRBM131300"
  		(pin_numbers
  			(hide yes)
  		)
  		(pin_names
  			(offset 1.27)
  		)
  		(exclude_from_sim no)
  		(in_bom yes)
  		(on_board yes)
  		(property "Reference" "SW"
  			(at 7.62 1.27 0)
  		)
  		(property "Value" "${FAMILY}"
  			(at 5.08 -2.032 0)
  		)
  		(property "Footprint" ""
  			(at 0 0 0)
  		)
  		(property "Datasheet" ""
  			(at 0 0 0)
  		)
  		(property "Description" "2 Poles 3 Ways Rotary Switch"
  			(at 0 0 0)
  		)
  		(symbol "SW_ALPS_SRBM131300_1_0"
  			(text "5"
  				(at -2.54 -3.81 0)
  			)
  			(text "4"
  				(at -2.54 -6.35 0)
  			)
  			(text "3"
  				(at -2.54 -8.89 0)
  			)
  			(text "2"
  				(at -2.54 -11.43 0)
  			)
  			(text "FRONT"
  				(at 7.62 -1.905 0)
  			)
  			(text "1"
  				(at 20.32 -8.89 0)
  			)
  			(pin bidirectional line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "NC")
  				(number "F5")
  			)
  			(pin bidirectional line
  				(at -5.08 -7.62 0)
  				(length 5.08)
  				(name "P3")
  				(number "F4")
  			)
  			(pin bidirectional line
  				(at -5.08 -10.16 0)
  				(length 5.08)
  				(name "P2")
  				(number "F3")
  			)
  			(pin bidirectional line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "P1")
  				(number "F2")
  			)
  			(pin bidirectional line
  				(at 20.32 -10.16 180)
  				(length 5.08)
  				(name "C")
  				(number "F1")
  			)
  		)
  		(symbol "SW_ALPS_SRBM131300_2_0"
  			(text "4"
  				(at -2.54 -3.81 0)
  			)
  			(text "3"
  				(at -2.54 -6.35 0)
  			)
  			(text "2"
  				(at -2.54 -8.89 0)
  			)
  			(text "1"
  				(at -2.54 -11.43 0)
  			)
  			(text "REAR"
  				(at 7.62 -1.905 0)
  			)
  			(text "5"
  				(at 20.32 -8.89 0)
  			)
  			(pin bidirectional line
  				(at -5.08 -5.08 0)
  				(length 5.08)
  				(name "NC")
  				(number "R4")
  			)
  			(pin bidirectional line
  				(at -5.08 -7.62 0)
  				(length 5.08)
  				(name "P3")
  				(number "R3")
  			)
  			(pin bidirectional line
  				(at -5.08 -10.16 0)
  				(length 5.08)
  				(name "P2")
  				(number "R2")
  			)
  			(pin bidirectional line
  				(at -5.08 -12.7 0)
  				(length 5.08)
  				(name "P1")
  				(number "R1")
  			)
  			(pin bidirectional line
  				(at 20.32 -10.16 180)
  				(length 5.08)
  				(name "C")
  				(number "R5")
  			)
  		)
  		(embedded_fonts no)
  	)
)
