(footprint "SW_ALPS_SRBM140700"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "2 Poles, 4 Positions, Horizontal Rotary Switch, ALPS SRBM Series")
	(property "Reference" "REF**"
		(at -6.6 -6.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_ALPS_SRBM140700"
		(at -6.6 6.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr allow_missing_courtyard)
	(fp_text user "c"
		(at -2.5431 4.60782 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "c"
		(at 2.6569 -3.59218 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "P1"
		(at -3.025 2.873 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "c"
		(at -2.5431 4.60782 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Front"
		(at -3.49218 2.0681 90)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "P1"
		(at 2.35 4.623 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "c"
		(at 2.6569 -3.59218 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "P3"
		(at 2.175 0.648 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "P2"
		(at -3.05 0.473 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "P2"
		(at 2.275 2.973 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "P3"
		(at -3.1 -2.002 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "F1" thru_hole circle
		(at 0 5 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "F2" thru_hole circle
		(at 0 2.5 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "F3" thru_hole circle
		(at 0 0 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "F4" thru_hole circle
		(at 0 -2.5 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "F5" thru_hole circle
		(at 0 -5 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "R1" thru_hole circle
		(at 5 5 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "R2" thru_hole circle
		(at 5 2.5 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "R3" thru_hole circle
		(at 5 0 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "R4" thru_hole circle
		(at 5 -2.5 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(pad "R5" thru_hole circle
		(at 5 -5 180)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
	)
	(embedded_fonts no)
)
