(footprint "SW_APEM_MU-AS90R"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Multidirectional Switch 5 Way (4-directional and center push)")
	(property "Reference" "REF**"
		(at 0 -6.275 0)
		(layer "F.SilkS")
	)
	(property "Value" "SW_APEM_MU-AS90R"
		(at 0 6.275 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(pad "" np_thru_hole circle
		(at -2.25 2.25)
		(size 0.5 0.5)
		(drill 1)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 0.25)
		(thermal_bridge_angle 90)
	)
	(pad "" np_thru_hole circle
		(at 2.25 2.25)
		(size 0.5 0.5)
		(drill 1)
		(layers "F&B.Cu" "*.Mask")
		(solder_mask_margin 0.25)
		(thermal_bridge_angle 90)
	)
	(pad "1" smd rect
		(at -6.3 -3.25)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6.3 0.45)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.3 3.25)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at 6.3 3.25)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 6.3 0.45)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 6.3 -3.25)
		(size 2 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
)
